<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="120.0688" y1="80.7176" x2="20.0688" y2="80.7176" width="0" layer="20"/>
<wire x1="20.0688" y1="80.7176" x2="20.0688" y2="0.7176" width="0" layer="20"/>
<wire x1="20.0688" y1="0.7176" x2="120.0688" y2="0.7176" width="0" layer="20"/>
<wire x1="120.0688" y1="0.7176" x2="120.0688" y2="80.7176" width="0" layer="20"/>
<text>https://cryptech.is/
Alpha rev02</text>
<text>rev 02</text>
<text>5V</text>
<text>GND</text>
<text>3V3</text>
<text>GND
pad</text>
<text>NOISY
DIODE</text>
<text>3V3</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>GND</text>
<text>RST</text>
<text>SCK</text>
<text>MISO</text>
<text>GND</text>
<text>SI</text>
<text>3V3</text>
<text>GND</text>
<text>BAT</text>
<text>3V3</text>
<text>PANIC</text>
<text>PANIC
!!!!!!!!!!!!!!</text>
<text>SWD</text>
<text>KILL MISO</text>
<text>2  PWR</text>
<text>15 GND</text>
<text>NRST</text>
<text>CLK</text>
<text>IO</text>
<text>GND</text>
<text>3V3</text>
</plain>
<libraries>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L_COPPER">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="_0603MP">
<description>&lt;b&gt;0603 MicroPitch&lt;/b&gt;</description>
</package>
<package name="CRYSTAL_3.2X2.5">
<description>3.2mm x 2.5mm Thin SMT Crystal</description>
</package>
</packages>
</library>
<library name="WE-SHC">
<packages>
<package name="WE-SHC_36103205_NO_CREAM">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
<package name="2X3_LOCK">
</package>
<package name="1X10_LOCK">
</package>
<package name="POWER_JACK_SMD">
</package>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="Panasonic-EXB-ERJ">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cad_tools/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="RESCAXE80P320X160X60-8N">
</package>
</packages>
</library>
<library name="MC74HC1G14DTT1G">
<packages>
<package name="SOT95P275X110-5N">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
<package name="NX3225">
</package>
<package name="XTAL3215">
</package>
</packages>
</library>
<library name="STM32-SWD-connector">
<packages>
<package name="100MIL_THT">
<description>100 mil spaced pads for STM32 SWD</description>
</package>
</packages>
</library>
<library name="UsedComponents">
<packages>
<package name="TACTILE_SWITCH">
<description>Tactile SMD mounted switch</description>
</package>
<package name="1206">
<description>SMD Multilayer</description>
</package>
<package name="RCLAMP0502A">
<description>&lt;b&gt;RCLAMP0502A&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="ATMEL-ATTINY828R-AU">
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="Microchip-23K640-I_SN">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="MCP79412">
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ASF">
<description>&lt;b&gt;CRYSTAL CLOCK OSCILLATORS&lt;/b&gt;&lt;p&gt;
5.0 Vdc or 3.3 Vdc - LOW PROFILE ULTRA MINIATURE CERAMIC SURFACE MOUNT&lt;br&gt;
Source: http://www.abracon.com/Oscillators/asf1-L-L1.pdf</description>
</package>
</packages>
</library>
<library name="Xilinx_XC7A200TFBG484">
<packages>
<package name="FF484">
<description>&lt;b&gt;FF484 FBG484&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="altera-configdevices">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA08-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistors_gaui">
<description>&lt;b&gt;2N7002T; N-channel TrenchMOS FET&lt;/b&gt;&lt;p&gt;
Produced by Philips. All information is found at:&lt;br&gt;
http://www.semiconductors.philips.com/pip/2N7002T.html&lt;br&gt;
&lt;/p&gt;
&lt;author&gt;Created by gudjon@mc2.chalmers.se&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Alpha-Power">
<packages>
<package name="QFN38_4X7X1.85">
</package>
<package name="QFN68_8X11X1.85">
<description>Altera EN5364QI 68-pin QFP</description>
</package>
<package name="NDY">
<description>NDY(11)</description>
</package>
<package name="TSOT-8-23">
</package>
</packages>
</library>
<library name="rc-master">
<description>&lt;b&gt;R/C MASTER! - v1.07 (07/03/2007)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD and through hole resistors and capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;p&gt;&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;
&lt;/author&gt;</description>
<packages>
<package name="CE-035X080">
<description>&lt;b&gt;POLCAP RADIAL&lt;/b&gt;&lt;p&gt;
3.5 mm lead spacing, 8 mm diameter, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="Alpha-IC">
<packages>
<package name="TSOP2-86L">
<description>&lt;b&gt;TSOP2-86L&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="LQFP-208">
</package>
<package name="FT2323HL_LQFP48">
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L_COPPER" value="OSHW-LOGOL-COPPER"/>
<element name="C16" library="resistor" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="Q2" library="transistor-npn" package="SOT23-BEC" value="BC818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="SOT23" value="BC847">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="resistor" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="R10" library="resistor" package="R0402" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R11" library="resistor" package="R0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="TP1" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="WE-SHC" package="WE-SHC_36103205_NO_CREAM" value="SHIELDING CABINET"/>
<element name="C15" library="resistor" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="R12" library="resistor" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="T2" library="transistor" package="SOT23" value="BC847">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="resistor" package="R0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="D1" library="diode" package="SOT23" value="BAT54">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED11" library="led" package="CHIP-LED0603" value="BLUE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="led" package="CHIP-LED0603" value="GREEN">
<attribute name="VALUE"/>
</element>
<element name="LED12" library="led" package="CHIP-LED0603" value="YELLOW">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="led" package="CHIP-LED0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIP-LED0603" value="BLUE">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0603" value="GREEN">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIP-LED0603" value="YELLOW">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="Panasonic-EXB-ERJ" package="RESCAXE80P320X160X60-8N" value="330R">
<attribute name="PACKAGE" value="0603"/>
<attribute name="OC_NEWARK" value="65T9098 "/>
<attribute name="POWERRATING" value="0.063 W/element"/>
<attribute name="TOLERANCE" value="±5 %"/>
<attribute name="MPN" value="EXB38V331JV"/>
<attribute name="SUPPLIER" value="PANASONIC "/>
<attribute name="OC_FARNELL" value="2060095 "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="Panasonic-EXB-ERJ" package="RESCAXE80P320X160X60-8N" value="330R">
<attribute name="PACKAGE" value="0603"/>
<attribute name="OC_NEWARK" value="65T9098 "/>
<attribute name="POWERRATING" value="0.063 W/element"/>
<attribute name="TOLERANCE" value="±5 %"/>
<attribute name="MPN" value="EXB38V331JV"/>
<attribute name="SUPPLIER" value="PANASONIC "/>
<attribute name="OC_FARNELL" value="2060095 "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="MC74HC1G14DTT1G" package="SOT95P275X110-5N" value="MC74HC1G14DTT1G">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="71J5593"/>
<attribute name="MPN" value="MC74HC1G14DTT1G"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="1468757"/>
<attribute name="NAME"/>
</element>
<element name="U4" library="Alpha-IC" package="LQFP-208" value="STM32F429BIT6">
<attribute name="OC_FARNELL" value="2469581"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0402" value="5 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="C0G"/>
</element>
<element name="C17" library="rcl" package="C0402" value="5 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="C0G"/>
</element>
<element name="J1" library="STM32-SWD-connector" package="100MIL_THT" value="STM32-SWD">
<attribute name="NAME"/>
</element>
<element name="C26" library="resistor" package="C0805" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C27" library="resistor" package="C0805" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C45" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C43" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C41" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C39" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C37" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C35" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C33" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C31" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C32" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C30" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C29" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C28" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C46" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C44" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C42" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C40" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C38" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C36" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C34" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C21" library="resistor" package="C0603" value="1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C24" library="resistor" package="C0603" value="2.2 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C22" library="resistor" package="C0603" value="2.2 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="R15" library="resistor" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="U8" library="Alpha-IC" package="FT2323HL_LQFP48" value="FT232H_SERIAL">
<attribute name="OC_FARNELL" value="1870924"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="resistor" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C20" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="R14" library="resistor" package="R0402" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C76" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C74" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="R22" library="resistor" package="R0402" value="12k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R24" library="resistor" package="R0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R25" library="resistor" package="R0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="LED5" library="led" package="CHIP-LED0603" value="YELLOW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="CHIP-LED0603" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C78" library="resistor" package="C0402" value="5 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C75" library="resistor" package="C0402" value="5 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C72" library="resistor" package="C0603" value="4.7 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C73" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C82" library="resistor" package="C0603" value="4.7 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C83" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C79" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C77" library="resistor" package="C0805" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C81" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C80" library="resistor" package="C0805" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C84" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C85" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C86" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="FB2" library="microbuilder" package="_0603MP" value="600R 500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="microbuilder" package="_0603MP" value="600R 500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="USB-MINIB" value="HOST">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="microbuilder" package="CRYSTAL_3.2X2.5" value="12 MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOLERANCE" value="±30 ppm"/>
<attribute name="MPN" value="ABM8G-12.000MHZ-4Y-T3"/>
<attribute name="OC_FARNELL" value="2467837"/>
<attribute name="SUPPLIER" value="ABRACON"/>
</element>
<element name="U10" library="ATMEL-ATTINY828R-AU" package="QFP80P900X900X120-32N" value="ATTINY828R-AU">
<attribute name="SUPPLIER" value="ATMEL"/>
<attribute name="MPN" value="ATTINY828R-AU"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="OC_FARNELL" value="2249850"/>
<attribute name="OC_NEWARK" value="Unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="resistor" package="C0603" value="2.2 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C25" library="resistor" package="C0603" value="2.2 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="resistor" package="R0402" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U12" library="Microchip-23K640-I_SN" package="SOIC127P600X175-8N" value="23K640-I/SN">
<attribute name="SUPPLIER" value="MICROCHIP"/>
<attribute name="MPN" value="23K640-I/SN "/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_FARNELL" value="1695549 "/>
<attribute name="OC_NEWARK" value="71P4706 "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="resistor" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="resistor" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C102" library="resistor" package="C0805" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C104" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C103" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C106" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C107" library="resistor" package="C0402" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="JP6" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X10_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="UsedComponents" package="TACTILE_SWITCH" value="TACTILE_SWITCH">
<attribute name="OC_FARNELL" value="2425618"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="MCP79412" package="SOIC127P600X175-8N" value="MCP79412-I/SN">
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="MPN" value="MCP79412-I/SN"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_FARNELL" value="2103565"/>
<attribute name="OC_NEWARK" value="94T5863"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C71" library="resistor" package="C0402" value="5 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C70" library="resistor" package="C0402" value="5 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="U13" library="Xilinx_XC7A200TFBG484" package="FF484" value="XC7A200TFBG484">
<attribute name="MFR" value="Xilinx"/>
<attribute name="MPN" value="XC7A200T-1FBG484C"/>
<attribute name="OC_DIGIKEY" value="122-1871-ND"/>
</element>
<element name="C123" library="resistor" package="SMC_D" value="330 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="TANTALUM"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C140" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C125" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="IC3" library="altera-configdevices" package="SO08" value="N25Q128A13ES">
<attribute name="PRICE100_DIGIKEY" value="1.30470"/>
<attribute name="OC_FARNELL" value="2253682"/>
<attribute name="PRICE100_FARNELL" value="5.10"/>
<attribute name="OC_DIGIKEY" value="557-1562-ND"/>
</element>
<element name="R51" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="JP9" library="jumper" package="JP1" value=""/>
<element name="R50" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R35" library="resistor" package="R0402" value="1.0k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C133" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C127" library="resistor" package="SMC_D" value="330 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="TANTALUM"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="LED17" library="led" package="CHIP-LED0603" value="BLUE"/>
<element name="LED15" library="led" package="CHIP-LED0603" value="GREEN"/>
<element name="LED16" library="led" package="CHIP-LED0603" value="YELLOW"/>
<element name="LED14" library="led" package="CHIP-LED0603" value="RED"/>
<element name="R36" library="resistor" package="R0402" value="1.0k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R37" library="resistor" package="R0402" value="1.0k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R65" library="resistor" package="R0402" value="1.0k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="SV2" library="con-lstb" package="MA08-2" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="SV3" library="con-lstb" package="MA08-2" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="Q5" library="crystal" package="ASF" value="ASFL1">
<attribute name="MPN" value="ASFL1-50.000MHZ-EK-T"/>
<attribute name="OC_FARNELL" value="2467924"/>
<attribute name="MF" value="Abracon Corporation"/>
<attribute name="OC_NEWARK" value=""/>
</element>
<element name="C111" library="resistor" package="C0402" value="0.01 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="R49" library="resistor" package="R0402" value="0"/>
<element name="R41" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R40" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="Q4" library="transistors_gaui" package="SOT23" value="2N7002"/>
<element name="R42" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="LED13" library="led" package="CHIP-LED0603" value="RED"/>
<element name="R38" library="resistor" package="R0402" value="330">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R39" library="resistor" package="R0402" value="100">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="SV1" library="con-lstb" package="MA08-1" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R43" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R44" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R45" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C113" library="resistor" package="C1210" value="22 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="R53" library="resistor" package="R0402" value="62k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R52" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R56" library="resistor" package="R0402" value="205k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R57" library="resistor" package="R0402" value="147k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="U14" library="Alpha-Power" package="QFN38_4X7X1.85" value="EN6347QI">
<attribute name="MPN" value="EN6347QI"/>
<attribute name="OC_FARNELL" value="2081146"/>
<attribute name="SUPPLIER" value="ENPIRION"/>
<attribute name="PACKAGE" value="QFN"/>
</element>
<element name="R60" library="resistor" package="R0402" value="470">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="FB5" library="UsedComponents" package="1206" value="0">
<attribute name="MPN" value="BLM31PG330SN1"/>
<attribute name="SUPPLIER" value="MURATA"/>
<attribute name="PACKAGE" value="1206"/>
</element>
<element name="C114" library="resistor" package="C1210" value="22 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="R55" library="resistor" package="R0402" value="62k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R54" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R58" library="resistor" package="R0402" value="205k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R59" library="resistor" package="R0402" value="59k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="U15" library="Alpha-Power" package="QFN38_4X7X1.85" value="EN6347QI">
<attribute name="MPN" value="EN6347QI"/>
<attribute name="OC_FARNELL" value="2081146"/>
<attribute name="SUPPLIER" value="ENPIRION"/>
<attribute name="PACKAGE" value="QFN"/>
</element>
<element name="R61" library="resistor" package="R0402" value="470">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="FB6" library="UsedComponents" package="1206" value="0">
<attribute name="MPN" value="BLM31PG330SN1"/>
<attribute name="SUPPLIER" value="MURATA"/>
<attribute name="PACKAGE" value="1206"/>
</element>
<element name="C207" library="resistor" package="C0402" value="0.047 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="R66" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C205" library="resistor" package="C1210" value="22 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C206" library="resistor" package="C1210" value="22 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="R68" library="resistor" package="R0402" value="150k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R69" library="resistor" package="R0402" value="226k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="C208" library="resistor" package="C0402" value="27pF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="U16" library="Alpha-Power" package="QFN68_8X11X1.85" value="EN5364QI">
<attribute name="MPN" value="EN5364QI"/>
<attribute name="OC_FARNELL" value="2081142"/>
<attribute name="SUPPLIER" value="ENPIRION"/>
<attribute name="PACKAGE" value="QFN"/>
</element>
<element name="FB7" library="UsedComponents" package="1206" value="0">
<attribute name="MPN" value="BLM31PG330SN1"/>
<attribute name="SUPPLIER" value="MURATA"/>
<attribute name="PACKAGE" value="1206"/>
</element>
<element name="R70" library="resistor" package="R0402" value="100">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R72" library="resistor" package="R0402" value="100k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="D2" library="diode" package="SOT23" value="BAT54"/>
<element name="R75" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R76" library="resistor" package="R0402" value="100k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="D4" library="diode" package="SOT23" value="BAT54"/>
<element name="R73" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R74" library="resistor" package="R0402" value="100k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="D3" library="diode" package="SOT23" value="BAT54"/>
<element name="R77" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="Q6" library="transistors_gaui" package="SOT23" value="2N7002"/>
<element name="LED18" library="led" package="CHIP-LED0603" value="GREEN"/>
<element name="R78" library="resistor" package="R0402" value="330">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="U1" library="Alpha-Power" package="NDY" value="LMZ13608">
<attribute name="MPN" value="LMZ13608TZ/NOPB"/>
<attribute name="OC_FARNELL" value="2492265"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="PACKAGE" value="NDY (11)"/>
</element>
<element name="C5" library="resistor" package="C0603" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="R3" library="resistor" package="R0402" value="100">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R2" library="resistor" package="R0402" value="4.64k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R1" library="resistor" package="R0402" value="56k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="C1" library="resistor" package="C1210" value="10 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="R8" library="resistor" package="R0402" value="6.3k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R9" library="resistor" package="R0402" value="1.21k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="C9" library="rc-master" package="CE-035X080" value="330 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C6" library="resistor" package="C0402" value="0.047 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C10" library="rc-master" package="CE-035X080" value="330 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C115" library="resistor" package="C0402" value="0.047 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C116" library="resistor" package="C0402" value="0.047 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C4" library="resistor" package="C0402" value="0.047 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="R67" library="resistor" package="R0402" value="0"/>
<element name="C109" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C124" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C128" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C130" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C134" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C129" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C131" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C135" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C138" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C142" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C146" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C150" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C154" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C158" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C162" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C163" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C143" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C147" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C151" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C155" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C159" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C181" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C187" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C193" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C199" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C182" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C188" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C194" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C200" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C183" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C189" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C195" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C201" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C184" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C190" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C196" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C202" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C185" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C191" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C197" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C203" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C186" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C192" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C198" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C204" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C164" library="resistor" package="C0402" value="0.47 uF">
<attribute name="RATED_VOLTAGE" value="6.3V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C118" library="resistor" package="C0402" value="27pF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C117" library="resistor" package="C0402" value="27pF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C108" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C112" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C121" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C122" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C211" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C212" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C213" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C2" library="resistor" package="C1210" value="10 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C3" library="resistor" package="C1210" value="10 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C144" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C148" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C152" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C156" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C160" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C141" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C145" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C149" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C153" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C157" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C161" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C132" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C136" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C139" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C169" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C175" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C176" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C170" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C171" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C177" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C178" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C172" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C173" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C179" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C180" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C174" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="10%"/>
</element>
<element name="C137" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C126" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C165" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C166" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C167" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C168" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C119" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C120" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C209" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C210" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="C8" library="resistor" package="C1210" value="47 uF">
<attribute name="RATED_VOLTAGE" value="16V"/>
<attribute name="DIELECTRIC" value="X5R"/>
<attribute name="TOLERANCE" value="20%"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="POWER_JACK_SMD" value="5.5x2.1mm Barrel">
<attribute name="SF_ID" value="PRT-12748"/>
<attribute name="PROD_ID" value="CONN-08106"/>
</element>
<element name="Q3" library="adafruit" package="NX3225" value="">
<attribute name="MPN" value="ABM8G-25.000MHZ-4Y-T3"/>
<attribute name="OC_FARNELL" value="2467848"/>
</element>
<element name="R64" library="Panasonic-EXB-ERJ" package="RESCAXE80P320X160X60-8N" value="330R">
<attribute name="POWERRATING" value="0.063 W/element"/>
<attribute name="OC_FARNELL" value="2060095 "/>
<attribute name="SUPPLIER" value="PANASONIC "/>
<attribute name="OC_NEWARK" value="65T9098 "/>
<attribute name="MPN" value="EXB38V331JV"/>
<attribute name="TOLERANCE" value="±5 %"/>
<attribute name="PACKAGE" value="0603"/>
</element>
<element name="X1" library="adafruit" package="XTAL3215" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="ABS07-32.768KHZ-T"/>
<attribute name="OC_FARNELL" value="2101347"/>
</element>
<element name="U2" library="Alpha-Power" package="TSOT-8-23" value="LT3060ITS8-15">
<attribute name="OC_FARNELL" value="2471073"/>
<attribute name="SUPPLIER" value=""/>
<attribute name="MPN" value="LT3060ITS8-15#TRMPBF"/>
</element>
<element name="C11" library="rcl" package="C0402" value="0.01 uF">
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="25V"/>
</element>
<element name="C12" library="rcl" package="C0402" value="0.01 uF">
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="25V"/>
</element>
<element name="C13" library="resistor" package="C0603" value="4.7 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="25V"/>
</element>
<element name="R7" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C19" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C105" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="R21" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R20" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R19" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="JP7" library="jumper" package="JP1" value=""/>
<element name="U5" library="Alpha-IC" package="TSOP2-86L" value="IS45S32160F">
<attribute name="MPN" value="IS45S32160F"/>
<attribute name="SUPPLIER" value="ISSI"/>
</element>
<element name="U9" library="Alpha-IC" package="FT2323HL_LQFP48" value="FT232H_SERIAL">
<attribute name="OC_FARNELL" value="1870924"/>
</element>
<element name="R27" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C91" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C89" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="R26" library="resistor" package="R0402" value="12k">
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R28" library="resistor" package="R0402" value="330">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R29" library="resistor" package="R0402" value="330">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="LED7" library="led" package="CHIP-LED0603" value="YELLOW"/>
<element name="LED8" library="led" package="CHIP-LED0603" value="GREEN"/>
<element name="C93" library="resistor" package="C0402" value="5 pF">
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C90" library="resistor" package="C0402" value="5 pF">
<attribute name="DIELECTRIC" value="C0G"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C87" library="resistor" package="C0603" value="4.7 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C88" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C97" library="resistor" package="C0603" value="4.7 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C98" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C94" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C92" library="resistor" package="C0805" value="10 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C96" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C95" library="resistor" package="C0805" value="10 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C99" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C100" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="C101" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="FB4" library="microbuilder" package="_0603MP" value="600R 500mA"/>
<element name="FB3" library="microbuilder" package="_0603MP" value="600R 500mA"/>
<element name="CN2" library="adafruit" package="USB-MINIB" value="HOST"/>
<element name="Y2" library="microbuilder" package="CRYSTAL_3.2X2.5" value="12 MHz">
<attribute name="TOLERANCE" value="±30 ppm"/>
<attribute name="OC_FARNELL" value="2467837"/>
<attribute name="MPN" value="ABM8G-12.000MHZ-4Y-T3"/>
<attribute name="SUPPLIER" value="ABRACON"/>
</element>
<element name="C56" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C54" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C52" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C50" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C51" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C49" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C48" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C47" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C57" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C55" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C53" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="U6" library="Alpha-IC" package="TSOP2-86L" value="IS45S32160F">
<attribute name="MPN" value="IS45S32160F"/>
<attribute name="SUPPLIER" value="ISSI"/>
</element>
<element name="C67" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C65" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C63" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C61" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C62" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C60" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C59" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C58" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C68" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C66" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C64" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="IC1" library="altera-configdevices" package="SO08" value="N25Q128A13ES">
<attribute name="OC_DIGIKEY" value="557-1562-ND"/>
<attribute name="OC_FARNELL" value="2253682"/>
<attribute name="PRICE100_DIGIKEY" value="1.30470"/>
<attribute name="PRICE100_FARNELL" value="5.10"/>
</element>
<element name="R18" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="C69" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="50V"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="Q1" library="transistors_gaui" package="SOT23" value="2N7002"/>
<element name="R6" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R5" library="resistor" package="R0402" value="1k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="JP2" library="jumper" package="JP1" value=""/>
<element name="C7" library="resistor" package="C0603" value="4.7 uF">
<attribute name="RATED_VOLTAGE" value="25V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="IC2" library="74xx-eu" package="SO20W" value="74AC244DW"/>
<element name="C110" library="resistor" package="C0402" value="0.1 uF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="RATED_VOLTAGE" value="10V"/>
</element>
<element name="R48" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R46" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R47" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="JP8" library="jumper" package="JP1" value=""/>
<element name="R4" library="resistor" package="R0402" value="0"/>
<element name="R17" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="IC4" library="74xx-eu" package="SO20W" value="74AC244DW"/>
<element name="R79" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R80" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R81" library="resistor" package="R0402" value="4.7k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R82" library="resistor" package="R0402" value="15k"/>
<element name="R32" library="resistor" package="R0402" value="0">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R62" library="resistor" package="R0603" value="0">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R63" library="resistor" package="R0603" value="0">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R71" library="resistor" package="R0603" value="0">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R83" library="resistor" package="R0603" value="0">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R84" library="resistor" package="R0603" value="0">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R85" library="resistor" package="R0603" value="0">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="IC5" library="UsedComponents" package="RCLAMP0502A" value="RCLAMP0502ASC-89">
<attribute name="OC_FARNELL" value="2058982"/>
<attribute name="MFR" value="SEMTECH"/>
<attribute name="MPN" value="RCLAMP0502A"/>
</element>
<element name="R86" library="resistor" package="R0402" value="100">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R87" library="resistor" package="R0402" value="100">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3-NS" value=""/>
<element name="C214" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="IC6" library="UsedComponents" package="RCLAMP0502A" value="RCLAMP0502ASC-89">
<attribute name="OC_FARNELL" value="2058982"/>
<attribute name="MFR" value="SEMTECH"/>
<attribute name="MPN" value="RCLAMP0502A"/>
</element>
<element name="R88" library="resistor" package="R0402" value="100">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R89" library="resistor" package="R0402" value="100">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="2X3-NS" value=""/>
<element name="C215" library="resistor" package="C0402" value="0.1 uF">
<attribute name="RATED_VOLTAGE" value="10V"/>
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="R90" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R91" library="resistor" package="R0402" value="10k">
<attribute name="TOLERANCE" value="5%"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="U8" pad="10"/>
<contactref element="U8" pad="11"/>
<contactref element="U8" pad="22"/>
<contactref element="U8" pad="23"/>
<contactref element="U8" pad="35"/>
<contactref element="U8" pad="36"/>
<contactref element="U8" pad="47"/>
<contactref element="C20" pad="2"/>
<contactref element="C76" pad="2"/>
<contactref element="C74" pad="2"/>
<contactref element="U8" pad="48"/>
<contactref element="U8" pad="4"/>
<contactref element="U8" pad="9"/>
<contactref element="U8" pad="41"/>
<contactref element="U8" pad="42"/>
<contactref element="C75" pad="1"/>
<contactref element="C78" pad="1"/>
<contactref element="C73" pad="2"/>
<contactref element="C79" pad="2"/>
<contactref element="C81" pad="2"/>
<contactref element="C84" pad="2"/>
<contactref element="C86" pad="2"/>
<contactref element="C85" pad="2"/>
<contactref element="CN1" pad="GND"/>
<contactref element="J1" pad="P$GND"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED11" pad="C"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED10" pad="C"/>
<contactref element="U10" pad="5"/>
<contactref element="U10" pad="21"/>
<contactref element="JP3" pad="6"/>
<contactref element="U12" pad="4"/>
<contactref element="C107" pad="2"/>
<contactref element="C102" pad="2"/>
<contactref element="C104" pad="2"/>
<contactref element="C103" pad="2"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP5" pad="10"/>
<contactref element="S2" pad="G1"/>
<contactref element="S2" pad="G2"/>
<contactref element="S2" pad="B2"/>
<contactref element="S2" pad="B1"/>
<contactref element="JP4" pad="3"/>
<contactref element="U7" pad="4"/>
<contactref element="C71" pad="1"/>
<contactref element="C70" pad="1"/>
<contactref element="U13" pad="A2"/>
<contactref element="U13" pad="A3"/>
<contactref element="U13" pad="A5"/>
<contactref element="U13" pad="A7"/>
<contactref element="U13" pad="A9"/>
<contactref element="U13" pad="A11"/>
<contactref element="U13" pad="A12"/>
<contactref element="U13" pad="A22"/>
<contactref element="U13" pad="B3"/>
<contactref element="U13" pad="B12"/>
<contactref element="U13" pad="B19"/>
<contactref element="U13" pad="C3"/>
<contactref element="U13" pad="C6"/>
<contactref element="U13" pad="C10"/>
<contactref element="U13" pad="C12"/>
<contactref element="U13" pad="C16"/>
<contactref element="U13" pad="D3"/>
<contactref element="U13" pad="D4"/>
<contactref element="U13" pad="D8"/>
<contactref element="U13" pad="D12"/>
<contactref element="U13" pad="D13"/>
<contactref element="U13" pad="E4"/>
<contactref element="U13" pad="E5"/>
<contactref element="U13" pad="E7"/>
<contactref element="U13" pad="E9"/>
<contactref element="U13" pad="E11"/>
<contactref element="U13" pad="E20"/>
<contactref element="U13" pad="F5"/>
<contactref element="U13" pad="F11"/>
<contactref element="U13" pad="F17"/>
<contactref element="U13" pad="G5"/>
<contactref element="U13" pad="G6"/>
<contactref element="U13" pad="G7"/>
<contactref element="U13" pad="G8"/>
<contactref element="U13" pad="G9"/>
<contactref element="U13" pad="G10"/>
<contactref element="U13" pad="G12"/>
<contactref element="U13" pad="G14"/>
<contactref element="U13" pad="H1"/>
<contactref element="U13" pad="H7"/>
<contactref element="U13" pad="H9"/>
<contactref element="U13" pad="H11"/>
<contactref element="U13" pad="H21"/>
<contactref element="U13" pad="J8"/>
<contactref element="U13" pad="J10"/>
<contactref element="U13" pad="J12"/>
<contactref element="U13" pad="J18"/>
<contactref element="U13" pad="K5"/>
<contactref element="U13" pad="K7"/>
<contactref element="U13" pad="K11"/>
<contactref element="U13" pad="K15"/>
<contactref element="U13" pad="L2"/>
<contactref element="U13" pad="L8"/>
<contactref element="U13" pad="L22"/>
<contactref element="U13" pad="M7"/>
<contactref element="U13" pad="M11"/>
<contactref element="U13" pad="M19"/>
<contactref element="U13" pad="N6"/>
<contactref element="U13" pad="N8"/>
<contactref element="U13" pad="N16"/>
<contactref element="U13" pad="P3"/>
<contactref element="U13" pad="P7"/>
<contactref element="U13" pad="P9"/>
<contactref element="U13" pad="P11"/>
<contactref element="U13" pad="P13"/>
<contactref element="U13" pad="R8"/>
<contactref element="U13" pad="R10"/>
<contactref element="U13" pad="R12"/>
<contactref element="U13" pad="R20"/>
<contactref element="U13" pad="T7"/>
<contactref element="U13" pad="T9"/>
<contactref element="U13" pad="T11"/>
<contactref element="U13" pad="T17"/>
<contactref element="U13" pad="U4"/>
<contactref element="U13" pad="U14"/>
<contactref element="U13" pad="V1"/>
<contactref element="U13" pad="V11"/>
<contactref element="U13" pad="V21"/>
<contactref element="U13" pad="W8"/>
<contactref element="U13" pad="W18"/>
<contactref element="U13" pad="Y5"/>
<contactref element="U13" pad="Y15"/>
<contactref element="U13" pad="AA2"/>
<contactref element="U13" pad="AA12"/>
<contactref element="U13" pad="AA22"/>
<contactref element="U13" pad="AB9"/>
<contactref element="U13" pad="AB19"/>
<contactref element="Q5" pad="2"/>
<contactref element="U13" pad="K9"/>
<contactref element="U13" pad="L9"/>
<contactref element="U13" pad="M10"/>
<contactref element="C109" pad="2"/>
<contactref element="U13" pad="N9"/>
<contactref element="U13" pad="N10"/>
<contactref element="U13" pad="E12"/>
<contactref element="C123" pad="-"/>
<contactref element="C127" pad="-"/>
<contactref element="C141" pad="2"/>
<contactref element="C145" pad="2"/>
<contactref element="C149" pad="2"/>
<contactref element="C153" pad="2"/>
<contactref element="C157" pad="2"/>
<contactref element="C161" pad="2"/>
<contactref element="C140" pad="2"/>
<contactref element="C144" pad="2"/>
<contactref element="C148" pad="2"/>
<contactref element="C152" pad="2"/>
<contactref element="C156" pad="2"/>
<contactref element="C160" pad="2"/>
<contactref element="C133" pad="2"/>
<contactref element="C137" pad="2"/>
<contactref element="C134" pad="2"/>
<contactref element="C130" pad="2"/>
<contactref element="C128" pad="2"/>
<contactref element="C124" pad="2"/>
<contactref element="C135" pad="2"/>
<contactref element="C131" pad="2"/>
<contactref element="C129" pad="2"/>
<contactref element="C125" pad="2"/>
<contactref element="C150" pad="2"/>
<contactref element="C146" pad="2"/>
<contactref element="C142" pad="2"/>
<contactref element="C138" pad="2"/>
<contactref element="C163" pad="2"/>
<contactref element="C162" pad="2"/>
<contactref element="C158" pad="2"/>
<contactref element="C154" pad="2"/>
<contactref element="C164" pad="2"/>
<contactref element="C126" pad="2"/>
<contactref element="C132" pad="2"/>
<contactref element="C136" pad="2"/>
<contactref element="C139" pad="2"/>
<contactref element="C147" pad="2"/>
<contactref element="C143" pad="2"/>
<contactref element="C151" pad="2"/>
<contactref element="C155" pad="2"/>
<contactref element="C159" pad="2"/>
<contactref element="C165" pad="2"/>
<contactref element="C166" pad="2"/>
<contactref element="C167" pad="2"/>
<contactref element="C168" pad="2"/>
<contactref element="C169" pad="2"/>
<contactref element="C175" pad="2"/>
<contactref element="C181" pad="2"/>
<contactref element="C187" pad="2"/>
<contactref element="C193" pad="2"/>
<contactref element="C199" pad="2"/>
<contactref element="C170" pad="2"/>
<contactref element="C176" pad="2"/>
<contactref element="C182" pad="2"/>
<contactref element="C188" pad="2"/>
<contactref element="C194" pad="2"/>
<contactref element="C200" pad="2"/>
<contactref element="C171" pad="2"/>
<contactref element="C177" pad="2"/>
<contactref element="C183" pad="2"/>
<contactref element="C189" pad="2"/>
<contactref element="C195" pad="2"/>
<contactref element="C201" pad="2"/>
<contactref element="C172" pad="2"/>
<contactref element="C178" pad="2"/>
<contactref element="C184" pad="2"/>
<contactref element="C190" pad="2"/>
<contactref element="C196" pad="2"/>
<contactref element="C202" pad="2"/>
<contactref element="C173" pad="2"/>
<contactref element="C179" pad="2"/>
<contactref element="C185" pad="2"/>
<contactref element="C191" pad="2"/>
<contactref element="C197" pad="2"/>
<contactref element="C203" pad="2"/>
<contactref element="C174" pad="2"/>
<contactref element="C180" pad="2"/>
<contactref element="C186" pad="2"/>
<contactref element="C192" pad="2"/>
<contactref element="C198" pad="2"/>
<contactref element="C204" pad="2"/>
<contactref element="IC3" pad="4"/>
<contactref element="R50" pad="1"/>
<contactref element="C112" pad="2"/>
<contactref element="R35" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="C121" pad="2"/>
<contactref element="SV2" pad="11"/>
<contactref element="SV2" pad="5"/>
<contactref element="SV2" pad="12"/>
<contactref element="SV2" pad="6"/>
<contactref element="C122" pad="2"/>
<contactref element="SV3" pad="11"/>
<contactref element="SV3" pad="5"/>
<contactref element="SV3" pad="12"/>
<contactref element="SV3" pad="6"/>
<contactref element="C111" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="R42" pad="1"/>
<contactref element="SV1" pad="8"/>
<contactref element="SV1" pad="7"/>
<contactref element="SV1" pad="6"/>
<contactref element="C108" pad="2"/>
<contactref element="U14" pad="32"/>
<contactref element="U14" pad="13"/>
<contactref element="U14" pad="15"/>
<contactref element="U14" pad="16"/>
<contactref element="U14" pad="P$40"/>
<contactref element="U14" pad="18"/>
<contactref element="U14" pad="14"/>
<contactref element="U14" pad="P$39"/>
<contactref element="U14" pad="17"/>
<contactref element="C115" pad="2"/>
<contactref element="C113" pad="2"/>
<contactref element="R53" pad="1"/>
<contactref element="R57" pad="1"/>
<contactref element="C119" pad="2"/>
<contactref element="R60" pad="1"/>
<contactref element="U15" pad="32"/>
<contactref element="U15" pad="13"/>
<contactref element="U15" pad="15"/>
<contactref element="U15" pad="16"/>
<contactref element="U15" pad="P$40"/>
<contactref element="U15" pad="18"/>
<contactref element="U15" pad="14"/>
<contactref element="U15" pad="P$39"/>
<contactref element="U15" pad="17"/>
<contactref element="C116" pad="2"/>
<contactref element="C114" pad="2"/>
<contactref element="R55" pad="1"/>
<contactref element="R59" pad="1"/>
<contactref element="C120" pad="2"/>
<contactref element="R61" pad="1"/>
<contactref element="U16" pad="55"/>
<contactref element="U16" pad="1"/>
<contactref element="U16" pad="29"/>
<contactref element="U16" pad="30"/>
<contactref element="U16" pad="65"/>
<contactref element="U16" pad="31"/>
<contactref element="U16" pad="66"/>
<contactref element="U16" pad="67"/>
<contactref element="U16" pad="32"/>
<contactref element="U16" pad="68"/>
<contactref element="U16" pad="2"/>
<contactref element="U16" pad="3"/>
<contactref element="U16" pad="4"/>
<contactref element="U16" pad="P$69"/>
<contactref element="U16" pad="P$70"/>
<contactref element="U16" pad="27"/>
<contactref element="U16" pad="28"/>
<contactref element="U16" pad="P$71"/>
<contactref element="U16" pad="64"/>
<contactref element="U16" pad="33"/>
<contactref element="C207" pad="2"/>
<contactref element="C205" pad="2"/>
<contactref element="C206" pad="2"/>
<contactref element="LED17" pad="C"/>
<contactref element="R69" pad="1"/>
<contactref element="C209" pad="2"/>
<contactref element="C210" pad="2"/>
<contactref element="R70" pad="1"/>
<contactref element="C211" pad="2"/>
<contactref element="C213" pad="2"/>
<contactref element="C212" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="U1" pad="TP1"/>
<contactref element="U1" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="-"/>
<contactref element="C10" pad="-"/>
<contactref element="JP1" pad="P$4"/>
<contactref element="T1" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="Q3" pad="4"/>
<contactref element="Q3" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C19" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="C83" pad="2"/>
<contactref element="C82" pad="2"/>
<contactref element="C77" pad="2"/>
<contactref element="C80" pad="2"/>
<contactref element="C72" pad="2"/>
<contactref element="C105" pad="2"/>
<contactref element="LED15" pad="C"/>
<contactref element="LED16" pad="C"/>
<contactref element="LED14" pad="C"/>
<contactref element="U9" pad="10"/>
<contactref element="U9" pad="11"/>
<contactref element="U9" pad="22"/>
<contactref element="U9" pad="23"/>
<contactref element="U9" pad="35"/>
<contactref element="U9" pad="36"/>
<contactref element="U9" pad="47"/>
<contactref element="U9" pad="48"/>
<contactref element="CN2" pad="GND"/>
<contactref element="C91" pad="2"/>
<contactref element="C89" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="U9" pad="4"/>
<contactref element="U9" pad="9"/>
<contactref element="U9" pad="41"/>
<contactref element="U9" pad="42"/>
<contactref element="C90" pad="1"/>
<contactref element="C93" pad="1"/>
<contactref element="C88" pad="2"/>
<contactref element="C87" pad="2"/>
<contactref element="C98" pad="2"/>
<contactref element="C97" pad="2"/>
<contactref element="C94" pad="2"/>
<contactref element="C92" pad="2"/>
<contactref element="C96" pad="2"/>
<contactref element="C95" pad="2"/>
<contactref element="C99" pad="2"/>
<contactref element="C101" pad="2"/>
<contactref element="C100" pad="2"/>
<contactref element="U5" pad="86"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="12"/>
<contactref element="U5" pad="32"/>
<contactref element="U5" pad="38"/>
<contactref element="U5" pad="46"/>
<contactref element="U5" pad="52"/>
<contactref element="U5" pad="78"/>
<contactref element="U5" pad="84"/>
<contactref element="U5" pad="44"/>
<contactref element="U5" pad="58"/>
<contactref element="U5" pad="72"/>
<contactref element="C47" pad="2"/>
<contactref element="C56" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="U6" pad="86"/>
<contactref element="U6" pad="6"/>
<contactref element="U6" pad="12"/>
<contactref element="U6" pad="32"/>
<contactref element="U6" pad="38"/>
<contactref element="U6" pad="46"/>
<contactref element="U6" pad="52"/>
<contactref element="U6" pad="78"/>
<contactref element="U6" pad="84"/>
<contactref element="U6" pad="44"/>
<contactref element="U6" pad="58"/>
<contactref element="U6" pad="72"/>
<contactref element="C58" pad="2"/>
<contactref element="C67" pad="2"/>
<contactref element="C65" pad="2"/>
<contactref element="C63" pad="2"/>
<contactref element="C61" pad="2"/>
<contactref element="C59" pad="2"/>
<contactref element="C68" pad="2"/>
<contactref element="C66" pad="2"/>
<contactref element="C64" pad="2"/>
<contactref element="C62" pad="2"/>
<contactref element="C60" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C69" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U4" pad="40"/>
<contactref element="U4" pad="14"/>
<contactref element="U4" pad="25"/>
<contactref element="U4" pad="51"/>
<contactref element="U4" pad="60"/>
<contactref element="U4" pad="72"/>
<contactref element="U4" pad="82"/>
<contactref element="U4" pad="93"/>
<contactref element="U4" pad="114"/>
<contactref element="U4" pad="125"/>
<contactref element="U4" pad="136"/>
<contactref element="U4" pad="149"/>
<contactref element="U4" pad="170"/>
<contactref element="U4" pad="184"/>
<contactref element="U4" pad="202"/>
<contactref element="IC2" pad="10"/>
<contactref element="C110" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="C24" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="IC4" pad="10"/>
<contactref element="R81" pad="2"/>
<contactref element="C106" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="4"/>
<contactref element="IC5" pad="2"/>
<contactref element="C214" pad="2"/>
<contactref element="IC6" pad="2"/>
<contactref element="C215" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="AMPLIFIED">
<contactref element="U3" pad="2"/>
<contactref element="T2" pad="3"/>
<contactref element="R13" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="D1" pad="3"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="NOISE_OUT">
<contactref element="Q2" pad="B"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="NOISE_IN">
<contactref element="R10" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="Q2" pad="E"/>
</signal>
<signal name="RAW_NOISE">
<contactref element="R10" pad="1"/>
<contactref element="T1" pad="3"/>
<contactref element="R11" pad="2"/>
<contactref element="TP1" pad="TP"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="AMP_P1">
<contactref element="D1" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED11" pad="A"/>
<contactref element="R31" pad="4"/>
</signal>
<signal name="AVR_LED1">
<contactref element="R31" pad="5"/>
<contactref element="U10" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="LED9" pad="A"/>
<contactref element="R31" pad="3"/>
</signal>
<signal name="AVR_LED2">
<contactref element="R31" pad="6"/>
<contactref element="U10" pad="10"/>
</signal>
<signal name="N$15">
<contactref element="LED12" pad="A"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="AVR_LED3">
<contactref element="R31" pad="7"/>
<contactref element="U10" pad="11"/>
</signal>
<signal name="N$16">
<contactref element="LED10" pad="A"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="AVR_LED4">
<contactref element="R31" pad="8"/>
<contactref element="U10" pad="12"/>
</signal>
<signal name="N$17">
<contactref element="LED3" pad="A"/>
<contactref element="R16" pad="4"/>
</signal>
<signal name="ARM_LED1">
<contactref element="R16" pad="5"/>
<contactref element="U4" pad="65"/>
</signal>
<signal name="N$18">
<contactref element="LED1" pad="A"/>
<contactref element="R16" pad="3"/>
</signal>
<signal name="ARM_LED2">
<contactref element="R16" pad="6"/>
<contactref element="U4" pad="66"/>
</signal>
<signal name="N$19">
<contactref element="LED4" pad="A"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="ARM_LED3">
<contactref element="R16" pad="7"/>
<contactref element="U4" pad="67"/>
</signal>
<signal name="N$20">
<contactref element="LED2" pad="A"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="ARM_LED4">
<contactref element="R16" pad="8"/>
<contactref element="U4" pad="68"/>
</signal>
<signal name="AGND">
<contactref element="T2" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="C16" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="5"/>
<contactref element="S1" pad="6"/>
<contactref element="S1" pad="7"/>
<contactref element="S1" pad="8"/>
<contactref element="S1" pad="9"/>
<contactref element="S1" pad="10"/>
<contactref element="S1" pad="11"/>
<contactref element="S1" pad="12"/>
<contactref element="S1" pad="13"/>
<contactref element="S1" pad="14"/>
<contactref element="S1" pad="15"/>
<contactref element="S1" pad="16"/>
</signal>
<signal name="N$10">
</signal>
<signal name="FMC_D0">
<contactref element="U13" pad="T3"/>
<contactref element="U5" pad="2"/>
<contactref element="U6" pad="2"/>
<contactref element="U4" pad="116"/>
</signal>
<signal name="FMC_D1">
<contactref element="U13" pad="T1"/>
<contactref element="U5" pad="4"/>
<contactref element="U6" pad="4"/>
<contactref element="U4" pad="117"/>
</signal>
<signal name="FMC_D13">
<contactref element="U13" pad="AA1"/>
<contactref element="U5" pad="82"/>
<contactref element="U6" pad="82"/>
<contactref element="U4" pad="108"/>
</signal>
<signal name="FMC_D14">
<contactref element="U13" pad="AB1"/>
<contactref element="U5" pad="83"/>
<contactref element="U6" pad="83"/>
<contactref element="U4" pad="109"/>
</signal>
<signal name="FMC_D15">
<contactref element="U13" pad="AB3"/>
<contactref element="U5" pad="85"/>
<contactref element="U6" pad="85"/>
<contactref element="U4" pad="110"/>
</signal>
<signal name="FMC_D22">
<contactref element="U13" pad="AA4"/>
<contactref element="U5" pad="40"/>
<contactref element="U6" pad="40"/>
<contactref element="U4" pad="152"/>
</signal>
<signal name="FMC_D23">
<contactref element="U13" pad="V4"/>
<contactref element="U5" pad="42"/>
<contactref element="U6" pad="42"/>
<contactref element="U4" pad="153"/>
</signal>
<signal name="FMC_D24">
<contactref element="U13" pad="W4"/>
<contactref element="U5" pad="45"/>
<contactref element="U6" pad="45"/>
<contactref element="U4" pad="154"/>
</signal>
<signal name="FMC_D25">
<contactref element="U13" pad="R4"/>
<contactref element="U5" pad="47"/>
<contactref element="U6" pad="47"/>
<contactref element="U4" pad="155"/>
</signal>
<signal name="FMC_D26">
<contactref element="U13" pad="T4"/>
<contactref element="U5" pad="48"/>
<contactref element="U6" pad="48"/>
<contactref element="U4" pad="156"/>
</signal>
<signal name="FMC_A12">
<contactref element="U13" pad="Y14"/>
<contactref element="U5" pad="69"/>
<contactref element="U6" pad="69"/>
<contactref element="U4" pad="129"/>
</signal>
<signal name="FMC_A13">
<contactref element="U13" pad="AB11"/>
<contactref element="U4" pad="130"/>
</signal>
<signal name="FMC_A14">
<contactref element="U13" pad="AB12"/>
<contactref element="U5" pad="22"/>
<contactref element="U6" pad="22"/>
<contactref element="U4" pad="131"/>
</signal>
<signal name="FMC_A16">
<contactref element="U13" pad="AB10"/>
<contactref element="U4" pad="111"/>
</signal>
<signal name="FMC_A17">
<contactref element="U13" pad="AA10"/>
<contactref element="U4" pad="112"/>
</signal>
<signal name="FMC_A18">
<contactref element="U13" pad="AA11"/>
<contactref element="U4" pad="113"/>
</signal>
<signal name="FMC_NL">
<contactref element="U13" pad="R6"/>
<contactref element="U4" pad="196"/>
</signal>
<signal name="FMC_D28">
<contactref element="U13" pad="U5"/>
<contactref element="U5" pad="51"/>
<contactref element="U6" pad="51"/>
<contactref element="U4" pad="207"/>
</signal>
<signal name="FMC_D29">
<contactref element="U13" pad="W6"/>
<contactref element="U5" pad="53"/>
<contactref element="U6" pad="53"/>
<contactref element="U4" pad="208"/>
</signal>
<signal name="FMC_D27">
<contactref element="U13" pad="T5"/>
<contactref element="U5" pad="50"/>
<contactref element="U6" pad="50"/>
<contactref element="U4" pad="157"/>
</signal>
<signal name="FMC_D3">
<contactref element="U13" pad="U2"/>
<contactref element="U5" pad="7"/>
<contactref element="U6" pad="7"/>
<contactref element="U4" pad="165"/>
</signal>
<signal name="FMC_NOE">
<contactref element="U13" pad="T6"/>
<contactref element="U4" pad="168"/>
</signal>
<signal name="FMC_NWE">
<contactref element="U13" pad="AA6"/>
<contactref element="U4" pad="169"/>
</signal>
<signal name="FMC_NWAIT">
<contactref element="U13" pad="Y6"/>
<contactref element="U4" pad="172"/>
</signal>
<signal name="FMC_A19">
<contactref element="U13" pad="V10"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="FMC_A20">
<contactref element="U13" pad="W10"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="FMC_A21">
<contactref element="U13" pad="Y11"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="FMC_D30">
<contactref element="U13" pad="W5"/>
<contactref element="U5" pad="54"/>
<contactref element="U6" pad="54"/>
<contactref element="U4" pad="11"/>
</signal>
<signal name="FMC_D31">
<contactref element="U13" pad="U6"/>
<contactref element="U5" pad="56"/>
<contactref element="U6" pad="56"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="FMC_A0">
<contactref element="U13" pad="Y17"/>
<contactref element="U5" pad="25"/>
<contactref element="U6" pad="25"/>
<contactref element="U4" pad="16"/>
</signal>
<signal name="FMC_A1">
<contactref element="U13" pad="Y16"/>
<contactref element="U5" pad="26"/>
<contactref element="U6" pad="26"/>
<contactref element="U4" pad="17"/>
</signal>
<signal name="FMC_A2">
<contactref element="U13" pad="AA16"/>
<contactref element="U5" pad="27"/>
<contactref element="U6" pad="27"/>
<contactref element="U4" pad="18"/>
</signal>
<signal name="FMC_A3">
<contactref element="U13" pad="AB16"/>
<contactref element="U5" pad="60"/>
<contactref element="U6" pad="60"/>
<contactref element="U4" pad="22"/>
</signal>
<signal name="FMC_A4">
<contactref element="U13" pad="AB17"/>
<contactref element="U5" pad="61"/>
<contactref element="U6" pad="61"/>
<contactref element="U4" pad="23"/>
</signal>
<signal name="FMC_A5">
<contactref element="U13" pad="AA13"/>
<contactref element="U5" pad="62"/>
<contactref element="U6" pad="62"/>
<contactref element="U4" pad="24"/>
</signal>
<signal name="FMC_A6">
<contactref element="U13" pad="AB13"/>
<contactref element="U5" pad="63"/>
<contactref element="U6" pad="63"/>
<contactref element="U4" pad="71"/>
</signal>
<signal name="FMC_A7">
<contactref element="U13" pad="AA15"/>
<contactref element="U5" pad="64"/>
<contactref element="U6" pad="64"/>
<contactref element="U4" pad="74"/>
</signal>
<signal name="FMC_A8">
<contactref element="U13" pad="AB15"/>
<contactref element="U5" pad="65"/>
<contactref element="U6" pad="65"/>
<contactref element="U4" pad="75"/>
</signal>
<signal name="FMC_A9">
<contactref element="U13" pad="Y13"/>
<contactref element="U5" pad="66"/>
<contactref element="U6" pad="66"/>
<contactref element="U4" pad="76"/>
</signal>
<signal name="FMC_A10">
<contactref element="U13" pad="AA14"/>
<contactref element="U5" pad="24"/>
<contactref element="U6" pad="24"/>
<contactref element="U4" pad="77"/>
</signal>
<signal name="FMC_A11">
<contactref element="U13" pad="W14"/>
<contactref element="U5" pad="21"/>
<contactref element="U6" pad="21"/>
<contactref element="U4" pad="78"/>
</signal>
<signal name="FMC_D4">
<contactref element="U13" pad="V2"/>
<contactref element="U5" pad="8"/>
<contactref element="U6" pad="8"/>
<contactref element="U4" pad="79"/>
</signal>
<signal name="FMC_D20">
<contactref element="U13" pad="AB5"/>
<contactref element="U5" pad="37"/>
<contactref element="U6" pad="37"/>
<contactref element="U4" pad="102"/>
</signal>
<signal name="FMC_D19">
<contactref element="U13" pad="AA5"/>
<contactref element="U5" pad="36"/>
<contactref element="U6" pad="36"/>
<contactref element="U4" pad="101"/>
</signal>
<signal name="FMC_D18">
<contactref element="U13" pad="AA3"/>
<contactref element="U5" pad="34"/>
<contactref element="U6" pad="34"/>
<contactref element="U4" pad="100"/>
</signal>
<signal name="FMC_D17">
<contactref element="U13" pad="Y3"/>
<contactref element="U5" pad="33"/>
<contactref element="U6" pad="33"/>
<contactref element="U4" pad="99"/>
</signal>
<signal name="FMC_D16">
<contactref element="U13" pad="AB2"/>
<contactref element="U5" pad="31"/>
<contactref element="U6" pad="31"/>
<contactref element="U4" pad="98"/>
</signal>
<signal name="FMC_D12">
<contactref element="U13" pad="V3"/>
<contactref element="U5" pad="80"/>
<contactref element="U6" pad="80"/>
<contactref element="U4" pad="89"/>
</signal>
<signal name="FMC_D11">
<contactref element="U13" pad="U3"/>
<contactref element="U5" pad="79"/>
<contactref element="U6" pad="79"/>
<contactref element="U4" pad="88"/>
</signal>
<signal name="FMC_D10">
<contactref element="U13" pad="Y1"/>
<contactref element="U5" pad="76"/>
<contactref element="U5" pad="77"/>
<contactref element="U6" pad="76"/>
<contactref element="U6" pad="77"/>
<contactref element="U4" pad="87"/>
</signal>
<signal name="FMC_D9">
<contactref element="U13" pad="W1"/>
<contactref element="U4" pad="86"/>
</signal>
<signal name="FMC_D8">
<contactref element="U13" pad="Y2"/>
<contactref element="U5" pad="74"/>
<contactref element="U6" pad="74"/>
<contactref element="U4" pad="85"/>
</signal>
<signal name="FMC_D7">
<contactref element="U13" pad="W2"/>
<contactref element="U5" pad="13"/>
<contactref element="U6" pad="13"/>
<contactref element="U4" pad="84"/>
</signal>
<signal name="FMC_D6">
<contactref element="U13" pad="R2"/>
<contactref element="U5" pad="11"/>
<contactref element="U6" pad="11"/>
<contactref element="U4" pad="81"/>
</signal>
<signal name="FMC_D5">
<contactref element="U13" pad="R3"/>
<contactref element="U5" pad="10"/>
<contactref element="U6" pad="10"/>
<contactref element="U4" pad="80"/>
</signal>
<signal name="FMC_D21">
<contactref element="U13" pad="Y4"/>
<contactref element="U5" pad="39"/>
<contactref element="U6" pad="39"/>
<contactref element="U4" pad="151"/>
</signal>
<signal name="FMC_A15">
<contactref element="U13" pad="AA9"/>
<contactref element="U5" pad="23"/>
<contactref element="U6" pad="23"/>
<contactref element="U4" pad="132"/>
</signal>
<signal name="FMC_D2">
<contactref element="U13" pad="U1"/>
<contactref element="U5" pad="5"/>
<contactref element="U6" pad="5"/>
<contactref element="U4" pad="164"/>
</signal>
<signal name="FMC_NE1">
<contactref element="U13" pad="V5"/>
<contactref element="U4" pad="173"/>
</signal>
<signal name="OSC_OUT">
<contactref element="C18" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="U4" pad="33"/>
</signal>
<signal name="OSC_IN">
<contactref element="R14" pad="1"/>
<contactref element="U4" pad="32"/>
</signal>
<signal name="SWDIO">
<contactref element="J1" pad="P$SWDIO"/>
<contactref element="U4" pad="147"/>
</signal>
<signal name="SWDCLK">
<contactref element="J1" pad="P$SWDCLK"/>
<contactref element="U4" pad="159"/>
</signal>
<signal name="NRST">
<contactref element="J1" pad="P$NRST"/>
<contactref element="C20" pad="1"/>
<contactref element="U4" pad="34"/>
</signal>
<signal name="VCAP2">
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="U4" pad="148"/>
</signal>
<signal name="VCAP1">
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="U4" pad="92"/>
</signal>
<signal name="BOOT0">
<contactref element="U4" pad="197"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="FT_RESET">
<contactref element="U8" pad="34"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="C17" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="FT_VCCA">
<contactref element="U8" pad="37"/>
<contactref element="C76" pad="1"/>
</signal>
<signal name="FT_VCCORE">
<contactref element="U8" pad="38"/>
<contactref element="C74" pad="1"/>
</signal>
<signal name="USB_DP">
<contactref element="U8" pad="7"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="USB_DM">
<contactref element="U8" pad="6"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="FT_VREGIN">
<contactref element="U8" pad="40"/>
<contactref element="CN1" pad="VBUS"/>
<contactref element="C73" pad="1"/>
<contactref element="C72" pad="1"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="FT_REF">
<contactref element="U8" pad="5"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R24" pad="1"/>
<contactref element="LED5" pad="C"/>
</signal>
<signal name="N$26">
<contactref element="R25" pad="1"/>
<contactref element="LED6" pad="C"/>
</signal>
<signal name="FT_RXLED">
<contactref element="U8" pad="27"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="FT_TXLED">
<contactref element="U8" pad="28"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="FT_VCC3V3">
<contactref element="U8" pad="39"/>
<contactref element="R23" pad="2"/>
<contactref element="LED6" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="U8" pad="46"/>
<contactref element="U8" pad="24"/>
<contactref element="U8" pad="12"/>
<contactref element="C84" pad="1"/>
<contactref element="C85" pad="1"/>
<contactref element="C86" pad="1"/>
<contactref element="FB1" pad="1"/>
<contactref element="FB2" pad="1"/>
<contactref element="C82" pad="1"/>
<contactref element="C83" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="C78" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="C75" pad="2"/>
<contactref element="U8" pad="1"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="FT_TXD">
<contactref element="U4" pad="50"/>
<contactref element="R86" pad="1"/>
<contactref element="R91" pad="2"/>
</signal>
<signal name="FT_RXD">
<contactref element="U4" pad="45"/>
<contactref element="R87" pad="1"/>
</signal>
<signal name="FT_VPHY">
<contactref element="U8" pad="3"/>
<contactref element="C79" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="FB1" pad="2"/>
</signal>
<signal name="FT_VPLL">
<contactref element="U8" pad="8"/>
<contactref element="C81" pad="1"/>
<contactref element="C80" pad="1"/>
<contactref element="FB2" pad="2"/>
</signal>
<signal name="AVR_RESET">
<contactref element="JP3" pad="5"/>
<contactref element="U10" pad="29"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U12" pad="7"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="MKM_SCK">
<contactref element="U12" pad="6"/>
<contactref element="IC4" pad="16"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="MKM_MOSI">
<contactref element="U12" pad="5"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="MKM_CS_N">
<contactref element="U12" pad="1"/>
<contactref element="R34" pad="1"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC4" pad="18"/>
<contactref element="R79" pad="1"/>
</signal>
<signal name="MKM_MISO">
<contactref element="U12" pad="2"/>
<contactref element="IC4" pad="17"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="MKM_CONTROL_AVR_ENA">
<contactref element="U10" pad="15"/>
<contactref element="IC4" pad="1"/>
<contactref element="R80" pad="1"/>
</signal>
<signal name="MKM_AVR_SCK">
<contactref element="U10" pad="30"/>
<contactref element="JP3" pad="3"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="MKM_AVR_CS_N">
<contactref element="IC4" pad="2"/>
<contactref element="U10" pad="14"/>
</signal>
<signal name="MKM_FPGA_MOSI">
<contactref element="U13" pad="P19"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="MKM_FPGA_MISO">
<contactref element="U13" pad="R19"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="MKM_FPGA_SCK">
<contactref element="U13" pad="U21"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="MKM_FPGA_CS_N">
<contactref element="U13" pad="T21"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="MKM_AVR_MOSI">
<contactref element="U10" pad="27"/>
<contactref element="JP3" pad="4"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="MKM_AVR_MISO">
<contactref element="JP3" pad="1"/>
<contactref element="U10" pad="28"/>
<contactref element="JP6" pad="2"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="AVR_GPIO_0">
<contactref element="JP5" pad="2"/>
<contactref element="U10" pad="31"/>
</signal>
<signal name="AVR_GPIO_1">
<contactref element="JP5" pad="3"/>
<contactref element="U10" pad="32"/>
</signal>
<signal name="AVR_GPIO_2">
<contactref element="JP5" pad="4"/>
<contactref element="U10" pad="1"/>
</signal>
<signal name="AVR_GPIO_3">
<contactref element="JP5" pad="5"/>
<contactref element="U10" pad="2"/>
</signal>
<signal name="AVR_GPIO_4">
<contactref element="JP5" pad="6"/>
<contactref element="U10" pad="3"/>
</signal>
<signal name="AVR_GPIO_5">
<contactref element="JP5" pad="7"/>
<contactref element="U10" pad="6"/>
</signal>
<signal name="AVR_GPIO_6">
<contactref element="JP5" pad="8"/>
<contactref element="U10" pad="7"/>
</signal>
<signal name="AVR_GPIO_7">
<contactref element="JP5" pad="9"/>
<contactref element="U10" pad="8"/>
</signal>
<signal name="AVR_PANIC">
<contactref element="S2" pad="A2"/>
<contactref element="R82" pad="1"/>
</signal>
<signal name="3V3_BATT">
<contactref element="C107" pad="1"/>
<contactref element="C106" pad="1"/>
<contactref element="U10" pad="4"/>
<contactref element="JP3" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="U12" pad="8"/>
<contactref element="C103" pad="1"/>
<contactref element="C102" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="C104" pad="1"/>
<contactref element="U10" pad="18"/>
<contactref element="JP4" pad="2"/>
<contactref element="U7" pad="3"/>
<contactref element="IC4" pad="20"/>
<contactref element="R80" pad="2"/>
<contactref element="R79" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R82" pad="2"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="AVR_GPIO_ARM_1">
<contactref element="U4" pad="9"/>
<contactref element="U10" pad="19"/>
</signal>
<signal name="AVR_GPIO_ARM_0">
<contactref element="U4" pad="8"/>
<contactref element="U10" pad="17"/>
</signal>
<signal name="RTC_X1">
<contactref element="U7" pad="1"/>
<contactref element="C70" pad="2"/>
<contactref element="X1" pad="P$1"/>
</signal>
<signal name="RTC_X2">
<contactref element="U7" pad="2"/>
<contactref element="C71" pad="2"/>
<contactref element="X1" pad="P$2"/>
</signal>
<signal name="RTC_MFP">
<contactref element="U7" pad="7"/>
<contactref element="R21" pad="2"/>
<contactref element="U4" pad="47"/>
</signal>
<signal name="RTC_SCL">
<contactref element="U7" pad="6"/>
<contactref element="R20" pad="2"/>
<contactref element="U4" pad="48"/>
</signal>
<signal name="RTC_SDA">
<contactref element="U7" pad="5"/>
<contactref element="R19" pad="2"/>
<contactref element="U4" pad="49"/>
</signal>
<signal name="N$12">
</signal>
<signal name="USB_PWR_VBUS">
</signal>
<signal name="FPGA_VCCAUX_1V8">
<contactref element="C143" pad="1"/>
<contactref element="C147" pad="1"/>
<contactref element="C151" pad="1"/>
<contactref element="C155" pad="1"/>
<contactref element="C159" pad="1"/>
<contactref element="C132" pad="1"/>
<contactref element="C136" pad="1"/>
<contactref element="C139" pad="1"/>
<contactref element="C126" pad="1"/>
<contactref element="FB5" pad="2"/>
<contactref element="U13" pad="K10"/>
<contactref element="C109" pad="1"/>
<contactref element="U13" pad="H12"/>
<contactref element="U13" pad="R11"/>
<contactref element="U13" pad="P12"/>
<contactref element="U13" pad="M12"/>
<contactref element="U13" pad="K12"/>
</signal>
<signal name="FPGA_VCCINT_1V0">
<contactref element="C123" pad="+"/>
<contactref element="C140" pad="1"/>
<contactref element="C125" pad="1"/>
<contactref element="C133" pad="1"/>
<contactref element="C127" pad="+"/>
<contactref element="C124" pad="1"/>
<contactref element="C128" pad="1"/>
<contactref element="C130" pad="1"/>
<contactref element="C134" pad="1"/>
<contactref element="C129" pad="1"/>
<contactref element="C131" pad="1"/>
<contactref element="C135" pad="1"/>
<contactref element="C138" pad="1"/>
<contactref element="C142" pad="1"/>
<contactref element="C146" pad="1"/>
<contactref element="C150" pad="1"/>
<contactref element="C154" pad="1"/>
<contactref element="C158" pad="1"/>
<contactref element="C162" pad="1"/>
<contactref element="C163" pad="1"/>
<contactref element="C164" pad="1"/>
<contactref element="C144" pad="1"/>
<contactref element="C148" pad="1"/>
<contactref element="C152" pad="1"/>
<contactref element="C156" pad="1"/>
<contactref element="C160" pad="1"/>
<contactref element="C141" pad="1"/>
<contactref element="C145" pad="1"/>
<contactref element="C149" pad="1"/>
<contactref element="C153" pad="1"/>
<contactref element="C157" pad="1"/>
<contactref element="C161" pad="1"/>
<contactref element="C137" pad="1"/>
<contactref element="FB7" pad="2"/>
<contactref element="U13" pad="J11"/>
<contactref element="U13" pad="L11"/>
<contactref element="U13" pad="N11"/>
<contactref element="U13" pad="T10"/>
<contactref element="U13" pad="T8"/>
<contactref element="U13" pad="R9"/>
<contactref element="U13" pad="R7"/>
<contactref element="U13" pad="P10"/>
<contactref element="U13" pad="P8"/>
<contactref element="U13" pad="N7"/>
<contactref element="U13" pad="H8"/>
<contactref element="U13" pad="M8"/>
<contactref element="U13" pad="L7"/>
<contactref element="U13" pad="K8"/>
<contactref element="U13" pad="J9"/>
<contactref element="U13" pad="J7"/>
<contactref element="U13" pad="H10"/>
</signal>
<signal name="VCCO_3V3">
<contactref element="C181" pad="1"/>
<contactref element="C187" pad="1"/>
<contactref element="C193" pad="1"/>
<contactref element="C199" pad="1"/>
<contactref element="C182" pad="1"/>
<contactref element="C188" pad="1"/>
<contactref element="C194" pad="1"/>
<contactref element="C200" pad="1"/>
<contactref element="C183" pad="1"/>
<contactref element="C189" pad="1"/>
<contactref element="C195" pad="1"/>
<contactref element="C201" pad="1"/>
<contactref element="C184" pad="1"/>
<contactref element="C190" pad="1"/>
<contactref element="C196" pad="1"/>
<contactref element="C202" pad="1"/>
<contactref element="C185" pad="1"/>
<contactref element="C191" pad="1"/>
<contactref element="C197" pad="1"/>
<contactref element="C203" pad="1"/>
<contactref element="C186" pad="1"/>
<contactref element="C192" pad="1"/>
<contactref element="C198" pad="1"/>
<contactref element="C204" pad="1"/>
<contactref element="C169" pad="1"/>
<contactref element="C175" pad="1"/>
<contactref element="C176" pad="1"/>
<contactref element="C170" pad="1"/>
<contactref element="C171" pad="1"/>
<contactref element="C177" pad="1"/>
<contactref element="C178" pad="1"/>
<contactref element="C172" pad="1"/>
<contactref element="C173" pad="1"/>
<contactref element="C179" pad="1"/>
<contactref element="C180" pad="1"/>
<contactref element="C174" pad="1"/>
<contactref element="C165" pad="1"/>
<contactref element="C166" pad="1"/>
<contactref element="C167" pad="1"/>
<contactref element="C168" pad="1"/>
<contactref element="FB6" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="C16" pad="2"/>
<contactref element="C39" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="J1" pad="P$VCC"/>
<contactref element="JP4" pad="1"/>
<contactref element="U7" pad="8"/>
<contactref element="C19" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="R45" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="SV1" pad="1"/>
<contactref element="C108" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="U13" pad="F12"/>
<contactref element="U13" pad="T12"/>
<contactref element="U13" pad="U8"/>
<contactref element="R51" pad="2"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="7"/>
<contactref element="JP9" pad="2"/>
<contactref element="C112" pad="1"/>
<contactref element="C111" pad="1"/>
<contactref element="Q5" pad="4"/>
<contactref element="R49" pad="2"/>
<contactref element="U13" pad="N21"/>
<contactref element="U13" pad="L17"/>
<contactref element="U13" pad="G19"/>
<contactref element="U13" pad="H16"/>
<contactref element="U13" pad="J13"/>
<contactref element="U13" pad="K20"/>
<contactref element="U13" pad="C1"/>
<contactref element="U13" pad="F2"/>
<contactref element="U13" pad="H6"/>
<contactref element="U13" pad="J3"/>
<contactref element="U13" pad="M4"/>
<contactref element="U13" pad="N1"/>
<contactref element="U13" pad="AB4"/>
<contactref element="U13" pad="R5"/>
<contactref element="U13" pad="T2"/>
<contactref element="U13" pad="V6"/>
<contactref element="U13" pad="W3"/>
<contactref element="U13" pad="AA7"/>
<contactref element="U13" pad="V16"/>
<contactref element="U13" pad="W13"/>
<contactref element="U13" pad="Y10"/>
<contactref element="U13" pad="AA17"/>
<contactref element="U13" pad="AB14"/>
<contactref element="U13" pad="F22"/>
<contactref element="U13" pad="E15"/>
<contactref element="U13" pad="D18"/>
<contactref element="U13" pad="C21"/>
<contactref element="U13" pad="B14"/>
<contactref element="U13" pad="A17"/>
<contactref element="SV2" pad="3"/>
<contactref element="SV2" pad="2"/>
<contactref element="SV2" pad="4"/>
<contactref element="SV2" pad="1"/>
<contactref element="C121" pad="1"/>
<contactref element="SV3" pad="3"/>
<contactref element="SV3" pad="2"/>
<contactref element="SV3" pad="4"/>
<contactref element="SV3" pad="1"/>
<contactref element="C122" pad="1"/>
<contactref element="U13" pad="Y20"/>
<contactref element="U13" pad="U19"/>
<contactref element="U13" pad="T22"/>
<contactref element="U13" pad="R15"/>
<contactref element="U13" pad="P18"/>
<contactref element="U13" pad="M14"/>
<contactref element="R65" pad="2"/>
<contactref element="U5" pad="43"/>
<contactref element="U5" pad="29"/>
<contactref element="U5" pad="15"/>
<contactref element="U5" pad="81"/>
<contactref element="U5" pad="75"/>
<contactref element="U5" pad="55"/>
<contactref element="U5" pad="49"/>
<contactref element="U5" pad="41"/>
<contactref element="U5" pad="35"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="C52" pad="1"/>
<contactref element="C54" pad="1"/>
<contactref element="C56" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="C53" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="C57" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="U6" pad="43"/>
<contactref element="U6" pad="29"/>
<contactref element="U6" pad="15"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="81"/>
<contactref element="U6" pad="75"/>
<contactref element="U6" pad="55"/>
<contactref element="U6" pad="49"/>
<contactref element="U6" pad="41"/>
<contactref element="U6" pad="35"/>
<contactref element="U6" pad="3"/>
<contactref element="C58" pad="1"/>
<contactref element="C59" pad="1"/>
<contactref element="C61" pad="1"/>
<contactref element="C63" pad="1"/>
<contactref element="C65" pad="1"/>
<contactref element="C67" pad="1"/>
<contactref element="C60" pad="1"/>
<contactref element="C62" pad="1"/>
<contactref element="C64" pad="1"/>
<contactref element="C66" pad="1"/>
<contactref element="C68" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="7"/>
<contactref element="C69" pad="1"/>
<contactref element="U4" pad="158"/>
<contactref element="U4" pad="171"/>
<contactref element="U4" pad="185"/>
<contactref element="U4" pad="204"/>
<contactref element="U4" pad="150"/>
<contactref element="U4" pad="137"/>
<contactref element="U4" pad="124"/>
<contactref element="U4" pad="115"/>
<contactref element="U4" pad="103"/>
<contactref element="U4" pad="94"/>
<contactref element="U4" pad="83"/>
<contactref element="U4" pad="73"/>
<contactref element="U4" pad="59"/>
<contactref element="U4" pad="52"/>
<contactref element="U4" pad="39"/>
<contactref element="U4" pad="26"/>
<contactref element="U4" pad="15"/>
<contactref element="U4" pad="42"/>
<contactref element="U4" pad="41"/>
<contactref element="U4" pad="203"/>
<contactref element="IC2" pad="20"/>
<contactref element="C110" pad="1"/>
<contactref element="R48" pad="2"/>
<contactref element="R46" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C214" pad="1"/>
<contactref element="C215" pad="1"/>
<contactref element="R90" pad="1"/>
<contactref element="R91" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="FMC_CLK">
<contactref element="U13" pad="W11"/>
<contactref element="U4" pad="167"/>
</signal>
<signal name="FPGA_PROM_SCLK">
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="FPGA_PROM_MOSI">
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="KSM_PROM_CS_N">
<contactref element="IC1" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="U4" pad="61"/>
</signal>
<signal name="FPGA_PROM_MISO">
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="FPGA_PROM_W_N">
<contactref element="IC3" pad="3"/>
<contactref element="R50" pad="2"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="FPGA_IRQ_N_0">
<contactref element="U13" pad="F14"/>
<contactref element="U4" pad="122"/>
</signal>
<signal name="FPGA_IRQ_N_1">
<contactref element="U13" pad="F16"/>
<contactref element="U4" pad="123"/>
</signal>
<signal name="FPGA_IRQ_N_2">
<contactref element="U13" pad="E17"/>
<contactref element="U4" pad="174"/>
</signal>
<signal name="FPGA_IRQ_N_3">
<contactref element="U13" pad="C14"/>
<contactref element="U4" pad="175"/>
</signal>
<signal name="FPGA_GPIO_A_0">
<contactref element="U13" pad="C15"/>
<contactref element="SV2" pad="7"/>
</signal>
<signal name="FPGA_GPIO_A_1">
<contactref element="U13" pad="E13"/>
<contactref element="SV2" pad="8"/>
</signal>
<signal name="FPGA_GPIO_A_2">
<contactref element="U13" pad="E14"/>
<contactref element="SV2" pad="9"/>
</signal>
<signal name="FPGA_GPIO_A_3">
<contactref element="U13" pad="E16"/>
<contactref element="SV2" pad="10"/>
</signal>
<signal name="FPGA_GPIO_A_4">
<contactref element="U13" pad="D16"/>
<contactref element="SV2" pad="13"/>
</signal>
<signal name="FPGA_GPIO_A_5">
<contactref element="U13" pad="D14"/>
<contactref element="SV2" pad="14"/>
</signal>
<signal name="FPGA_GPIO_A_6">
<contactref element="U13" pad="D15"/>
<contactref element="SV2" pad="15"/>
</signal>
<signal name="FPGA_GPIO_A_7">
<contactref element="U13" pad="B15"/>
<contactref element="SV2" pad="16"/>
</signal>
<signal name="FPGA_GPIO_B_0">
<contactref element="U13" pad="B16"/>
<contactref element="SV3" pad="7"/>
</signal>
<signal name="FPGA_GPIO_B_1">
<contactref element="U13" pad="C13"/>
<contactref element="SV3" pad="8"/>
</signal>
<signal name="FPGA_GPIO_B_2">
<contactref element="U13" pad="B13"/>
<contactref element="SV3" pad="9"/>
</signal>
<signal name="FPGA_GPIO_B_3">
<contactref element="U13" pad="A15"/>
<contactref element="SV3" pad="10"/>
</signal>
<signal name="FPGA_GPIO_B_4">
<contactref element="U13" pad="A16"/>
<contactref element="SV3" pad="13"/>
</signal>
<signal name="FPGA_GPIO_B_5">
<contactref element="U13" pad="A13"/>
<contactref element="SV3" pad="14"/>
</signal>
<signal name="FPGA_GPIO_B_6">
<contactref element="U13" pad="A14"/>
<contactref element="SV3" pad="15"/>
</signal>
<signal name="FPGA_GPIO_B_7">
<contactref element="U13" pad="B17"/>
<contactref element="SV3" pad="16"/>
</signal>
<signal name="FPGA_GCLK">
<contactref element="U13" pad="D17"/>
</signal>
<signal name="DIGITIZED_NOISE">
<contactref element="U13" pad="W19"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="FPGA_GPIO_LED_2">
<contactref element="U13" pad="W22"/>
<contactref element="R64" pad="2"/>
</signal>
<signal name="FPGA_GPIO_LED_3">
<contactref element="U13" pad="AA20"/>
<contactref element="R64" pad="1"/>
</signal>
<signal name="FPGA_M2">
<contactref element="U13" pad="U9"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="FPGA_JTAG_TCK">
<contactref element="U13" pad="V12"/>
<contactref element="SV1" pad="2"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="FPGA_JTAG_TDI">
<contactref element="U13" pad="R13"/>
<contactref element="SV1" pad="4"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="FPGA_JTAG_TDO">
<contactref element="U13" pad="U13"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="FPGA_JTAG_TMS">
<contactref element="U13" pad="T13"/>
<contactref element="SV1" pad="3"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="FPGA_PROGRAM_B">
<contactref element="R41" pad="1"/>
<contactref element="U4" pad="120"/>
<contactref element="R63" pad="1"/>
</signal>
<signal name="FPGA_DONE_INT">
<contactref element="U13" pad="G11"/>
<contactref element="LED13" pad="C"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="FPGA_M0">
<contactref element="U13" pad="U11"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="FPGA_M1">
<contactref element="U13" pad="U10"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="FPGA_GPIO_LED_0">
<contactref element="U13" pad="T20"/>
<contactref element="R64" pad="4"/>
</signal>
<signal name="FPGA_GPIO_LED_1">
<contactref element="U13" pad="W21"/>
<contactref element="R64" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="LED17" pad="A"/>
<contactref element="R64" pad="5"/>
</signal>
<signal name="N$28">
<contactref element="LED15" pad="A"/>
<contactref element="R64" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="LED16" pad="A"/>
<contactref element="R64" pad="7"/>
</signal>
<signal name="N$30">
<contactref element="LED14" pad="A"/>
<contactref element="R64" pad="8"/>
</signal>
<signal name="N$32">
<contactref element="U13" pad="U22"/>
<contactref element="R65" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="Q5" pad="1"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="FPGA_INIT_B_INT">
<contactref element="R40" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="FPGA_INIT_B">
<contactref element="Q4" pad="1"/>
<contactref element="R42" pad="2"/>
<contactref element="U4" pad="119"/>
</signal>
<signal name="N$34">
<contactref element="R38" pad="1"/>
<contactref element="LED13" pad="A"/>
</signal>
<signal name="FPGA_DONE">
<contactref element="R39" pad="1"/>
<contactref element="U4" pad="177"/>
</signal>
<signal name="N$35">
<contactref element="U14" pad="30"/>
<contactref element="C115" pad="1"/>
</signal>
<signal name="VCC_5V0">
<contactref element="C205" pad="1"/>
<contactref element="C206" pad="1"/>
<contactref element="R66" pad="2"/>
<contactref element="U16" pad="35"/>
<contactref element="U16" pad="42"/>
<contactref element="U16" pad="38"/>
<contactref element="U16" pad="34"/>
<contactref element="U16" pad="40"/>
<contactref element="U16" pad="41"/>
<contactref element="U16" pad="36"/>
<contactref element="U16" pad="37"/>
<contactref element="U16" pad="43"/>
<contactref element="U16" pad="39"/>
<contactref element="U16" pad="53"/>
<contactref element="R72" pad="1"/>
<contactref element="D2" pad="3"/>
<contactref element="R75" pad="2"/>
<contactref element="R73" pad="2"/>
<contactref element="R77" pad="2"/>
<contactref element="R78" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="R8" pad="2"/>
<contactref element="C9" pad="+"/>
<contactref element="C10" pad="+"/>
<contactref element="C8" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="C113" pad="1"/>
<contactref element="R52" pad="2"/>
<contactref element="U14" pad="19"/>
<contactref element="U14" pad="20"/>
<contactref element="U14" pad="21"/>
<contactref element="U14" pad="33"/>
<contactref element="C114" pad="1"/>
<contactref element="R54" pad="2"/>
<contactref element="U15" pad="19"/>
<contactref element="U15" pad="20"/>
<contactref element="U15" pad="21"/>
<contactref element="U15" pad="33"/>
</signal>
<signal name="PWR_ENA_VCCAUX">
<contactref element="U14" pad="27"/>
<contactref element="R76" pad="2"/>
<contactref element="D4" pad="1"/>
<contactref element="C213" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R53" pad="2"/>
<contactref element="U14" pad="29"/>
</signal>
<signal name="N$37">
<contactref element="R52" pad="1"/>
<contactref element="U14" pad="26"/>
</signal>
<signal name="N$38">
<contactref element="U14" pad="9"/>
<contactref element="U14" pad="5"/>
<contactref element="U14" pad="11"/>
<contactref element="U14" pad="7"/>
<contactref element="U14" pad="8"/>
<contactref element="U14" pad="10"/>
<contactref element="U14" pad="6"/>
<contactref element="R56" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="FB5" pad="1"/>
<contactref element="C117" pad="1"/>
<contactref element="C119" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="R56" pad="1"/>
<contactref element="U14" pad="31"/>
<contactref element="R57" pad="2"/>
<contactref element="C117" pad="2"/>
</signal>
<signal name="POK_VCCINT">
<contactref element="U16" pad="54"/>
<contactref element="R75" pad="1"/>
<contactref element="R76" pad="1"/>
<contactref element="D4" pad="3"/>
</signal>
<signal name="N$40">
<contactref element="U15" pad="30"/>
<contactref element="C116" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="R55" pad="2"/>
<contactref element="U15" pad="29"/>
</signal>
<signal name="N$42">
<contactref element="R54" pad="1"/>
<contactref element="U15" pad="26"/>
</signal>
<signal name="N$43">
<contactref element="U15" pad="9"/>
<contactref element="U15" pad="5"/>
<contactref element="U15" pad="11"/>
<contactref element="U15" pad="7"/>
<contactref element="U15" pad="8"/>
<contactref element="U15" pad="10"/>
<contactref element="U15" pad="6"/>
<contactref element="R58" pad="2"/>
<contactref element="R61" pad="2"/>
<contactref element="FB6" pad="1"/>
<contactref element="C118" pad="1"/>
<contactref element="C120" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="R58" pad="1"/>
<contactref element="U15" pad="31"/>
<contactref element="R59" pad="2"/>
<contactref element="C118" pad="2"/>
</signal>
<signal name="PWR_ENA_VCCO">
<contactref element="U15" pad="27"/>
<contactref element="D3" pad="1"/>
<contactref element="R74" pad="2"/>
<contactref element="C212" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="C207" pad="1"/>
<contactref element="U16" pad="59"/>
</signal>
<signal name="N$46">
<contactref element="R66" pad="1"/>
<contactref element="U16" pad="51"/>
</signal>
<signal name="PWR_ENA_VCCINT">
<contactref element="U16" pad="52"/>
<contactref element="D2" pad="1"/>
<contactref element="R72" pad="2"/>
<contactref element="C211" pad="1"/>
</signal>
<signal name="POK_VCCAUX">
<contactref element="U14" pad="28"/>
<contactref element="R73" pad="1"/>
<contactref element="R74" pad="1"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="POK_VCCO">
<contactref element="U15" pad="28"/>
<contactref element="R77" pad="1"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="U16" pad="63"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="U16" pad="7"/>
<contactref element="U16" pad="11"/>
<contactref element="U16" pad="10"/>
<contactref element="U16" pad="6"/>
<contactref element="U16" pad="8"/>
<contactref element="U16" pad="12"/>
<contactref element="U16" pad="13"/>
<contactref element="U16" pad="9"/>
<contactref element="U16" pad="5"/>
<contactref element="R68" pad="2"/>
<contactref element="C208" pad="1"/>
<contactref element="R70" pad="2"/>
<contactref element="FB7" pad="1"/>
<contactref element="R67" pad="2"/>
<contactref element="C209" pad="1"/>
<contactref element="C210" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="U16" pad="56"/>
<contactref element="R68" pad="1"/>
<contactref element="R69" pad="2"/>
<contactref element="C208" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="Q6" pad="3"/>
<contactref element="LED18" pad="C"/>
</signal>
<signal name="N$51">
<contactref element="R78" pad="1"/>
<contactref element="LED18" pad="A"/>
</signal>
<signal name="N$52">
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="PWR_18V">
<contactref element="JP1" pad="VIN0"/>
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$56">
<contactref element="U1" pad="7"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="FMC_A22">
<contactref element="U13" pad="Y12"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="FMC_A23">
<contactref element="U13" pad="W12"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="FMC_A24">
<contactref element="U13" pad="V13"/>
<contactref element="U4" pad="182"/>
</signal>
<signal name="FMC_A25">
<contactref element="U13" pad="V14"/>
<contactref element="U4" pad="183"/>
</signal>
<signal name="15V_STABLE">
<contactref element="R11" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C11" pad="1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="C12" pad="2"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="15V_LDO_ENABLE">
<contactref element="U2" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="VIN">
</signal>
<signal name="VOUT">
</signal>
<signal name="FT_RTS">
<contactref element="U8" pad="15"/>
<contactref element="U4" pad="43"/>
</signal>
<signal name="FT_CTS">
<contactref element="U8" pad="16"/>
<contactref element="U4" pad="44"/>
</signal>
<signal name="FT_DTR">
<contactref element="U8" pad="17"/>
<contactref element="U4" pad="53"/>
</signal>
<signal name="VCC">
<contactref element="JP5" pad="1"/>
<contactref element="C105" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="FPGA_CFG_SCLK">
<contactref element="IC2" pad="13"/>
<contactref element="R71" pad="1"/>
</signal>
<signal name="FPGA_CFG_MOSI">
<contactref element="IC2" pad="15"/>
<contactref element="R83" pad="1"/>
</signal>
<signal name="FPGA_CFG_CS_N">
<contactref element="IC2" pad="11"/>
<contactref element="R85" pad="1"/>
</signal>
<signal name="FPGA_CFG_MISO">
<contactref element="IC2" pad="3"/>
<contactref element="R84" pad="1"/>
</signal>
<signal name="ARM_FPGA_CFG_MOSI">
<contactref element="U4" pad="107"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="ARM_FPGA_CFG_MISO">
<contactref element="U4" pad="106"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="ARM_FPGA_CFG_SCLK">
<contactref element="U4" pad="105"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="FPGA_CFG_CTRL_ARM_ENA">
<contactref element="JP7" pad="2"/>
<contactref element="U4" pad="118"/>
</signal>
<signal name="FT_RESET1">
<contactref element="U9" pad="34"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="FT_VCCA1">
<contactref element="U9" pad="37"/>
<contactref element="C91" pad="1"/>
</signal>
<signal name="FT_VCCORE1">
<contactref element="U9" pad="38"/>
<contactref element="C89" pad="1"/>
</signal>
<signal name="FT_REF1">
<contactref element="U9" pad="5"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R28" pad="1"/>
<contactref element="LED7" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="R29" pad="1"/>
<contactref element="LED8" pad="C"/>
</signal>
<signal name="FT_RXLED1">
<contactref element="U9" pad="27"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="FT_TXLED1">
<contactref element="U9" pad="28"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="C93" pad="2"/>
<contactref element="U9" pad="2"/>
<contactref element="Y2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="C90" pad="2"/>
<contactref element="U9" pad="1"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="FT_MGMT_VREGIN">
<contactref element="U9" pad="40"/>
<contactref element="C88" pad="1"/>
<contactref element="C87" pad="1"/>
<contactref element="IC6" pad="5"/>
<contactref element="CN2" pad="VBUS"/>
</signal>
<signal name="FT_MGMT_VCC3V3">
<contactref element="U9" pad="39"/>
<contactref element="R27" pad="2"/>
<contactref element="LED7" pad="A"/>
<contactref element="LED8" pad="A"/>
<contactref element="U9" pad="46"/>
<contactref element="U9" pad="24"/>
<contactref element="U9" pad="12"/>
<contactref element="C99" pad="1"/>
<contactref element="C100" pad="1"/>
<contactref element="C101" pad="1"/>
<contactref element="FB3" pad="1"/>
<contactref element="FB4" pad="1"/>
<contactref element="C97" pad="1"/>
<contactref element="C98" pad="1"/>
</signal>
<signal name="USB_MGMT_DP">
<contactref element="U9" pad="7"/>
<contactref element="IC6" pad="1"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="USB_MGMT_DM">
<contactref element="U9" pad="6"/>
<contactref element="IC6" pad="3"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="FT_MGMT_VPLL">
<contactref element="U9" pad="8"/>
<contactref element="C96" pad="1"/>
<contactref element="C95" pad="1"/>
<contactref element="FB4" pad="2"/>
</signal>
<signal name="FT_MGMT_VPHY">
<contactref element="U9" pad="3"/>
<contactref element="C94" pad="1"/>
<contactref element="C92" pad="1"/>
<contactref element="FB3" pad="2"/>
</signal>
<signal name="FT_MGMT_TXD">
<contactref element="U4" pad="144"/>
<contactref element="R88" pad="1"/>
<contactref element="R90" pad="2"/>
</signal>
<signal name="FT_MGMT_RXD">
<contactref element="U4" pad="143"/>
<contactref element="R89" pad="1"/>
</signal>
<signal name="FT_MGMT_RTS">
<contactref element="U9" pad="15"/>
<contactref element="U4" pad="145"/>
</signal>
<signal name="FT_MGMT_CTS">
<contactref element="U9" pad="16"/>
<contactref element="U4" pad="146"/>
</signal>
<signal name="FT_MGMT_DTR">
<contactref element="U9" pad="17"/>
<contactref element="U4" pad="142"/>
</signal>
<signal name="FMC_SDCKE0">
<contactref element="U5" pad="67"/>
<contactref element="U4" pad="38"/>
</signal>
<signal name="FMC_SDNE0">
<contactref element="U5" pad="20"/>
<contactref element="U4" pad="37"/>
</signal>
<signal name="FMC_SDNWE">
<contactref element="U5" pad="17"/>
<contactref element="U6" pad="17"/>
<contactref element="U4" pad="35"/>
</signal>
<signal name="FMC_SDNCAS">
<contactref element="U5" pad="18"/>
<contactref element="U6" pad="18"/>
<contactref element="U4" pad="191"/>
</signal>
<signal name="FMC_SDNRAS">
<contactref element="U5" pad="19"/>
<contactref element="U6" pad="19"/>
<contactref element="U4" pad="70"/>
</signal>
<signal name="FMC_NBL0">
<contactref element="U5" pad="16"/>
<contactref element="U6" pad="16"/>
<contactref element="U4" pad="200"/>
</signal>
<signal name="FMC_NBL1">
<contactref element="U5" pad="71"/>
<contactref element="U6" pad="71"/>
<contactref element="U4" pad="201"/>
</signal>
<signal name="FMC_NBL2">
<contactref element="U5" pad="28"/>
<contactref element="U6" pad="28"/>
<contactref element="U4" pad="205"/>
</signal>
<signal name="FMC_NBL3">
<contactref element="U5" pad="59"/>
<contactref element="U6" pad="59"/>
<contactref element="U4" pad="206"/>
</signal>
<signal name="FMC_SDCLK">
<contactref element="U5" pad="68"/>
<contactref element="U6" pad="68"/>
<contactref element="U4" pad="135"/>
</signal>
<signal name="FMC_SDCKE1">
<contactref element="U6" pad="67"/>
<contactref element="U4" pad="194"/>
</signal>
<signal name="FMC_SDNE1">
<contactref element="U6" pad="20"/>
<contactref element="U4" pad="195"/>
</signal>
<signal name="KSM_PROM_MOSI">
<contactref element="IC1" pad="5"/>
<contactref element="U4" pad="56"/>
</signal>
<signal name="KSM_PROM_SCLK">
<contactref element="IC1" pad="6"/>
<contactref element="U4" pad="54"/>
</signal>
<signal name="KSM_PROM_MISO">
<contactref element="IC1" pad="2"/>
<contactref element="U4" pad="55"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="FPGA_ENTROPY_DISABLE">
<contactref element="R5" pad="1"/>
<contactref element="U13" pad="B18"/>
</signal>
<signal name="ARM_FPGA_CFG_CS_N">
<contactref element="IC2" pad="2"/>
<contactref element="U4" pad="104"/>
</signal>
<signal name="SPI_A_TRISTATE">
<contactref element="IC2" pad="1"/>
<contactref element="R46" pad="1"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="SPI_B_TRISTATE">
<contactref element="IC2" pad="19"/>
<contactref element="R47" pad="1"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="FPGA_PROM_CS_N">
<contactref element="IC3" pad="1"/>
<contactref element="R51" pad="1"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="18"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="FPGA_CFG_CTRL_FPGA_DIS">
<contactref element="JP8" pad="2"/>
<contactref element="U4" pad="95"/>
</signal>
<signal name="N$3">
<contactref element="Q5" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="3"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="MKM_CONTROL_FPGA_DIS">
<contactref element="IC4" pad="19"/>
<contactref element="R81" pad="1"/>
</signal>
<signal name="AVR_GPIO_ARM_3">
</signal>
<signal name="AVR_GPIO_FPGA_2">
<contactref element="U10" pad="25"/>
</signal>
<signal name="AVR_GPIO_FPGA_3">
<contactref element="U10" pad="26"/>
</signal>
<signal name="N$25">
<contactref element="U4" pad="6"/>
</signal>
<signal name="N$53">
<contactref element="R32" pad="2"/>
</signal>
<signal name="FPGA_INIT_B_INT1">
<contactref element="U13" pad="U12"/>
<contactref element="R62" pad="2"/>
</signal>
<signal name="FPGA_PROGRAM_B1">
<contactref element="U13" pad="N12"/>
<contactref element="R63" pad="2"/>
</signal>
<signal name="FPGA_CFG_SCLK1">
<contactref element="U13" pad="L12"/>
<contactref element="R71" pad="2"/>
</signal>
<signal name="FPGA_CFG_MISO1">
<contactref element="U13" pad="R22"/>
<contactref element="R84" pad="2"/>
</signal>
<signal name="FPGA_CFG_MOSI1">
<contactref element="U13" pad="P22"/>
<contactref element="R83" pad="2"/>
</signal>
<signal name="FPGA_CFG_CS_N1">
<contactref element="U13" pad="T19"/>
<contactref element="R85" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="IC5" pad="6"/>
<contactref element="CN1" pad="D+"/>
</signal>
<signal name="N$58">
<contactref element="IC5" pad="4"/>
<contactref element="CN1" pad="D-"/>
</signal>
<signal name="FT_TXD1">
<contactref element="R86" pad="2"/>
<contactref element="U8" pad="13"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="FT_RXD1">
<contactref element="R87" pad="2"/>
<contactref element="U8" pad="14"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$59">
<contactref element="IC6" pad="6"/>
<contactref element="CN2" pad="D+"/>
</signal>
<signal name="N$60">
<contactref element="IC6" pad="4"/>
<contactref element="CN2" pad="D-"/>
</signal>
<signal name="FT_MGMT_TXD1">
<contactref element="R88" pad="2"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="FT_MGMT_RXD1">
<contactref element="R89" pad="2"/>
<contactref element="J3" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
