<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<packages>
<package name="TSOP2-86L">
<description>&lt;b&gt;TSOP2-86L&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="LQFP-208">
</package>
<package name="FT2323HL_LQFP48">
</package>
</packages>
<symbols>
<symbol name="IS45S32160F-TSOP86L">
<pin name="VDD@1" direction="pwr"/>
<pin name="DQ0"/>
<pin name="VDDQ@3" direction="pwr"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="VSSQ@6" direction="pwr"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="VSSQ@12" direction="pwr"/>
<pin name="DQ7"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="DQM0"/>
<pin name="!WE" direction="in"/>
<pin name="!CAS"/>
<pin name="!RAS"/>
<pin name="!CS" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="BA0"/>
<pin name="BA1"/>
<pin name="A10" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="DQM2"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="DQ16"/>
<pin name="VSSQ@32" direction="pwr"/>
<pin name="DQ17"/>
<pin name="DQ18"/>
<pin name="VDDQ@35" direction="pwr"/>
<pin name="DQ19"/>
<pin name="DQ20"/>
<pin name="VSSQ@38" direction="pwr"/>
<pin name="DQ21"/>
<pin name="DQ22"/>
<pin name="VDDQ@41" direction="pwr"/>
<pin name="DQ23"/>
<pin name="VDD@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="DQ24"/>
<pin name="VSSQ@46" direction="pwr"/>
<pin name="DQ25"/>
<pin name="DQ26"/>
<pin name="VDDQ@49" direction="pwr"/>
<pin name="DQ27"/>
<pin name="DQ28"/>
<pin name="VSSQ@52" direction="pwr"/>
<pin name="DQ29"/>
<pin name="DQ30"/>
<pin name="VDDQ@55" direction="pwr"/>
<pin name="DQ31"/>
<pin name="VSS@58" direction="pwr"/>
<pin name="DQM3"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="CKE" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A12" direction="in"/>
<pin name="DQM1"/>
<pin name="VSS@72" direction="pwr"/>
<pin name="DQ8"/>
<pin name="VDDQ@75" direction="pwr"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="VSSQ@78" direction="pwr"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="VDDQ@81" direction="pwr"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="VSSQ@84" direction="pwr"/>
<pin name="DQ15"/>
<pin name="VSS@86" direction="pwr"/>
</symbol>
<symbol name="STM32F429_LQFP-208_IO">
<description>STM32 ARM GPIO</description>
<pin name="PI8"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PI11"/>
<pin name="PI12"/>
<pin name="PI13"/>
<pin name="PI14"/>
<pin name="FMC_NIORD/PF6"/>
<pin name="FMC_NREG/PF7"/>
<pin name="FMC_NIOWR/PF8"/>
<pin name="FMC_CD/PF9"/>
<pin name="FMC_INTR/PF10"/>
<pin name="PC1"/>
<pin name="USART2_CTS/WKUP/PA0"/>
<pin name="USART2_RTS/PA1"/>
<pin name="USART2_TX/PA2"/>
<pin name="FMC_SDCKE0/PH2"/>
<pin name="PH3"/>
<pin name="I2C2_SCL/PH4"/>
<pin name="I2C2_SDA/PH5"/>
<pin name="USART2_RX/PA3"/>
<pin name="PA4"/>
<pin name="SPI1_SCK/PA5"/>
<pin name="SPI1_MISO/PA6"/>
<pin name="SPI1_MOSI/PA7"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PI15"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PJ5"/>
<pin name="FMC_SDNE1/PH6"/>
<pin name="FMC_SDCKE1/PH7"/>
<pin name="PB12"/>
<pin name="SPI2_SCK/PB13"/>
<pin name="SPI2_MISO/PB14"/>
<pin name="SPI2_MOSI/PB15"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PJ8"/>
<pin name="PJ9"/>
<pin name="PJ10"/>
<pin name="PJ11"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="FMC_INT2/PG6"/>
<pin name="FMC_INT3/PG7"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="SDIO_D0/PC8"/>
<pin name="SDIO_D1/PC9"/>
<pin name="PA8"/>
<pin name="USART1_TX/PA9"/>
<pin name="USART1_RX/PA10"/>
<pin name="USART1_CTS/PA11"/>
<pin name="USART1_RTS/PA12"/>
<pin name="SDIO_D2/PC10"/>
<pin name="SDIO_D3/PC11"/>
<pin name="SDIO_CK/PC12"/>
<pin name="SDIO_CMD/PD2"/>
<pin name="PJ12"/>
<pin name="PJ13"/>
<pin name="PJ14"/>
<pin name="PJ15"/>
<pin name="FMC_NE2/FMC_NCE3/PG9"/>
<pin name="FMC_NCE4_1/FMC_NE3/PG10"/>
<pin name="FMC_NCE4_2/PG11"/>
<pin name="FMC_NE4/PG12"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
<pin name="PB8/I2C1_SCL"/>
<pin name="PB9/I2C1_SDA"/>
</symbol>
<symbol name="STM32F429_LQFP-208_CFG">
<description>Basic configuration for STM32</description>
<pin name="PA14/JTCK-SWCLK"/>
<pin name="PA15/JTDI"/>
<pin name="PB3/JTDO/TRACESWO"/>
<pin name="PB4/NJTRST"/>
<pin name="BOOT0@197" direction="in"/>
<pin name="PDR_ON@203"/>
<pin name="PA13/JTMS-SWDIO"/>
<pin name="OSC_IN/PH0"/>
<pin name="OSC_OUT/PH1"/>
<pin name="NRST" direction="in"/>
<pin name="VREF+@41" direction="pwr"/>
<pin name="PB2/BOOT1"/>
</symbol>
<symbol name="STM32F429_LQFP-208_PWR">
<pin name="VBAT@6" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@39" direction="pwr"/>
<pin name="VDDA@42" direction="pwr"/>
<pin name="VDD@52" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSSA@40" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VDD@59" direction="pwr"/>
<pin name="VDD@73" direction="pwr"/>
<pin name="VDD@83" direction="pwr"/>
<pin name="VDD@94" direction="pwr"/>
<pin name="VDD@103" direction="pwr"/>
<pin name="VSS@60" direction="pwr"/>
<pin name="VSS@72" direction="pwr"/>
<pin name="VSS@82" direction="pwr"/>
<pin name="VSS@93" direction="pwr"/>
<pin name="VDD@115" direction="pwr"/>
<pin name="VDD@124" direction="pwr"/>
<pin name="VDD@137" direction="pwr"/>
<pin name="VDD@150" direction="pwr"/>
<pin name="VSS@114" direction="pwr"/>
<pin name="VSS@125" direction="pwr"/>
<pin name="VSS@136" direction="pwr"/>
<pin name="VSS@149" direction="pwr"/>
<pin name="VDD@158" direction="pwr"/>
<pin name="VDD@171" direction="pwr"/>
<pin name="VDD@185" direction="pwr"/>
<pin name="VDD@204" direction="pwr"/>
<pin name="VSS@170" direction="pwr"/>
<pin name="VSS@184" direction="pwr"/>
<pin name="VSS@202" direction="pwr"/>
<pin name="VCAP1@92"/>
<pin name="VCAP2@148"/>
</symbol>
<symbol name="STM32F429_LQFP-208_FMC">
<description>The STM FMC bus</description>
<pin name="PH13/FMC_D21"/>
<pin name="PH14/FMC_D22"/>
<pin name="PH15/FMC_D23"/>
<pin name="PI0/FMC_D24"/>
<pin name="PI1/FMC_D25"/>
<pin name="PI2/FMC_D26"/>
<pin name="PE7/FMC_D4"/>
<pin name="PE8/FMC_D5"/>
<pin name="PE9/FMC_D6"/>
<pin name="PE10/FMC_D7"/>
<pin name="PE11/FMC_D8"/>
<pin name="PE12/FMC_D9"/>
<pin name="PE13/FMC_D10"/>
<pin name="PE14/FMC_D11"/>
<pin name="PE15/FMC_D12"/>
<pin name="PD8/FMC_D13"/>
<pin name="PD9/FMC_D14"/>
<pin name="PD10/FMC_D15"/>
<pin name="PD14/FMC_D0"/>
<pin name="PD15/FMC_D1"/>
<pin name="PD0/FMC_D2"/>
<pin name="PD1/FMC_D3"/>
<pin name="PI6/FMC_D28"/>
<pin name="PI7/FMC_D29"/>
<pin name="PH8/FMC_D16"/>
<pin name="PH9/FMC_D17"/>
<pin name="PH10/FMC_D18"/>
<pin name="PH11/FMC_D19"/>
<pin name="PH12/FMC_D20"/>
<pin name="PI9/FMC_D30"/>
<pin name="PI10/FMC_D31"/>
<pin name="PI3/FMC_D27"/>
<pin name="FMC_A23/PE2"/>
<pin name="FMC_A19/PE3"/>
<pin name="FMC_A20/PE4"/>
<pin name="FMC_A21/PE5"/>
<pin name="FMC_A22/PE6"/>
<pin name="FMC_A0/PF0"/>
<pin name="FMC_A1/PF1"/>
<pin name="FMC_A2/PF2"/>
<pin name="FMC_A3/PF3"/>
<pin name="FMC_A4/PF4"/>
<pin name="FMC_A5/PF5"/>
<pin name="FMC_A6/PF12"/>
<pin name="FMC_A7/PF13"/>
<pin name="FMC_A8/PF14"/>
<pin name="FMC_A9/PF15"/>
<pin name="FMC_A10/PG0"/>
<pin name="FMC_A11/PG1"/>
<pin name="FMC_A16/PD11"/>
<pin name="FMC_A17/PD12"/>
<pin name="FMC_A18/PD13"/>
<pin name="FMC_A12/PG2"/>
<pin name="FMC_A13/PG3"/>
<pin name="FMC_A14/PG4"/>
<pin name="FMC_A15/PG5"/>
<pin name="FMC_A24/PG13"/>
<pin name="FMC_A25/PG14"/>
<pin name="FMC_CLK/PD3"/>
<pin name="FMC_NOE/PD4"/>
<pin name="FMC_NWE/PD5"/>
<pin name="FMC_NWAIT/PD6"/>
<pin name="FMC_NE1/PD7"/>
<pin name="PG15/FMC_SDNCAS"/>
<pin name="PB5/FMC_SDCKE1"/>
<pin name="PB6/FMC_SDNE1"/>
<pin name="FMC_NL/PB7"/>
<pin name="FMC_NBL2/PI4"/>
<pin name="FMC_NBL3/PI5"/>
<pin name="FMC_NBL0/PE0"/>
<pin name="FMC_NBL1/PE1"/>
<pin name="PG8/FMC_SDCLK"/>
<pin name="PF11/FMC_SDNRAS"/>
<pin name="PC0/FMC_SDNWE"/>
<pin name="PC2/FMC_SDNE0"/>
<pin name="PC3/FMC_SDCKE0"/>
</symbol>
<symbol name="FT232H">
<pin name="VREGIN"/>
<pin name="VCCD" direction="pwr"/>
<pin name="VCCORE" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="!RESET" direction="in"/>
<pin name="REF"/>
<pin name="EECS"/>
<pin name="EECLK"/>
<pin name="EEDATA"/>
<pin name="XCSI"/>
<pin name="XCSO"/>
<pin name="TEST"/>
<pin name="ADBUS0"/>
<pin name="ADBUS1"/>
<pin name="ADBUS2"/>
<pin name="ADBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS5"/>
<pin name="ADBUS6"/>
<pin name="ADBUS7"/>
<pin name="ACBUS0"/>
<pin name="ACBUS1"/>
<pin name="ACBUS2"/>
<pin name="ACBUS3"/>
<pin name="ACBUS4"/>
<pin name="ACBUS5"/>
<pin name="ACBUS6"/>
<pin name="ACBUS7"/>
<pin name="ACBUS8"/>
<pin name="ACBUS9"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AGND@9" direction="pwr"/>
<pin name="AGND@41" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="VPHY"/>
<pin name="VPLL"/>
<pin name="VCCIO@12" direction="pwr"/>
<pin name="VCCIO@24" direction="pwr"/>
<pin name="VCCIO@46" direction="pwr"/>
</symbol>
<symbol name="FT232H_ASYNC_SERIAL">
<description>INTERFACE USB-UART in ASYNC SERIAL (RS232) MODE&lt;BR&gt;
12 Mbaud data transfer rate in this mode.</description>
<pin name="VREGIN" direction="pwr"/>
<pin name="VCCD" direction="pwr"/>
<pin name="VCCORE" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="!RESET" direction="in"/>
<pin name="REF"/>
<pin name="EECS" direction="out"/>
<pin name="EECLK" direction="out"/>
<pin name="EEDATA"/>
<pin name="XCSI"/>
<pin name="XCSO"/>
<pin name="TEST"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS#" direction="out"/>
<pin name="CTS#" direction="in"/>
<pin name="DTR#" direction="out"/>
<pin name="DSR#" direction="in"/>
<pin name="DCD#" direction="in"/>
<pin name="RI#" direction="in"/>
<pin name="TXDEN" direction="out"/>
<pin name="ACBUS1"/>
<pin name="ACBUS2"/>
<pin name="RXLED#" direction="out"/>
<pin name="TXLED#" direction="out"/>
<pin name="ACBUS5"/>
<pin name="ACBUS6"/>
<pin name="PWRSAV#"/>
<pin name="ACBUS8"/>
<pin name="ACBUS9"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AGND@9" direction="pwr"/>
<pin name="AGND@41" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="VPHY"/>
<pin name="VPLL"/>
<pin name="VCCIO@12" direction="pwr"/>
<pin name="VCCIO@24" direction="pwr"/>
<pin name="VCCIO@46" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="IS45S32160F" prefix="U">
<description>16Mx32, 512Mb SDRAM
Clock frequency: 166, 143 MHz</description>
<gates>
<gate name="G$1" symbol="IS45S32160F-TSOP86L"/>
</gates>
<devices>
<device name="" package="TSOP2-86L">
<connects>
<connect gate="G$1" pin="!CAS" pad="18"/>
<connect gate="G$1" pin="!CS" pad="20"/>
<connect gate="G$1" pin="!RAS" pad="19"/>
<connect gate="G$1" pin="!WE" pad="17"/>
<connect gate="G$1" pin="A0" pad="25"/>
<connect gate="G$1" pin="A1" pad="26"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A11" pad="21"/>
<connect gate="G$1" pin="A12" pad="69"/>
<connect gate="G$1" pin="A2" pad="27"/>
<connect gate="G$1" pin="A3" pad="60"/>
<connect gate="G$1" pin="A4" pad="61"/>
<connect gate="G$1" pin="A5" pad="62"/>
<connect gate="G$1" pin="A6" pad="63"/>
<connect gate="G$1" pin="A7" pad="64"/>
<connect gate="G$1" pin="A8" pad="65"/>
<connect gate="G$1" pin="A9" pad="66"/>
<connect gate="G$1" pin="BA0" pad="22"/>
<connect gate="G$1" pin="BA1" pad="23"/>
<connect gate="G$1" pin="CKE" pad="67"/>
<connect gate="G$1" pin="CLK" pad="68"/>
<connect gate="G$1" pin="DQ0" pad="2"/>
<connect gate="G$1" pin="DQ1" pad="4"/>
<connect gate="G$1" pin="DQ10" pad="77"/>
<connect gate="G$1" pin="DQ11" pad="79"/>
<connect gate="G$1" pin="DQ12" pad="80"/>
<connect gate="G$1" pin="DQ13" pad="82"/>
<connect gate="G$1" pin="DQ14" pad="83"/>
<connect gate="G$1" pin="DQ15" pad="85"/>
<connect gate="G$1" pin="DQ16" pad="31"/>
<connect gate="G$1" pin="DQ17" pad="33"/>
<connect gate="G$1" pin="DQ18" pad="34"/>
<connect gate="G$1" pin="DQ19" pad="36"/>
<connect gate="G$1" pin="DQ2" pad="5"/>
<connect gate="G$1" pin="DQ20" pad="37"/>
<connect gate="G$1" pin="DQ21" pad="39"/>
<connect gate="G$1" pin="DQ22" pad="40"/>
<connect gate="G$1" pin="DQ23" pad="42"/>
<connect gate="G$1" pin="DQ24" pad="45"/>
<connect gate="G$1" pin="DQ25" pad="47"/>
<connect gate="G$1" pin="DQ26" pad="48"/>
<connect gate="G$1" pin="DQ27" pad="50"/>
<connect gate="G$1" pin="DQ28" pad="51"/>
<connect gate="G$1" pin="DQ29" pad="53"/>
<connect gate="G$1" pin="DQ3" pad="7"/>
<connect gate="G$1" pin="DQ30" pad="54"/>
<connect gate="G$1" pin="DQ31" pad="56"/>
<connect gate="G$1" pin="DQ4" pad="8"/>
<connect gate="G$1" pin="DQ5" pad="10"/>
<connect gate="G$1" pin="DQ6" pad="11"/>
<connect gate="G$1" pin="DQ7" pad="13"/>
<connect gate="G$1" pin="DQ8" pad="74"/>
<connect gate="G$1" pin="DQ9" pad="76"/>
<connect gate="G$1" pin="DQM0" pad="16"/>
<connect gate="G$1" pin="DQM1" pad="71"/>
<connect gate="G$1" pin="DQM2" pad="28"/>
<connect gate="G$1" pin="DQM3" pad="59"/>
<connect gate="G$1" pin="VDD@1" pad="1"/>
<connect gate="G$1" pin="VDD@15" pad="15"/>
<connect gate="G$1" pin="VDD@29" pad="29"/>
<connect gate="G$1" pin="VDD@43" pad="43"/>
<connect gate="G$1" pin="VDDQ@3" pad="3"/>
<connect gate="G$1" pin="VDDQ@35" pad="35"/>
<connect gate="G$1" pin="VDDQ@41" pad="41"/>
<connect gate="G$1" pin="VDDQ@49" pad="49"/>
<connect gate="G$1" pin="VDDQ@55" pad="55"/>
<connect gate="G$1" pin="VDDQ@75" pad="75"/>
<connect gate="G$1" pin="VDDQ@81" pad="81"/>
<connect gate="G$1" pin="VSS@44" pad="44"/>
<connect gate="G$1" pin="VSS@58" pad="58"/>
<connect gate="G$1" pin="VSS@72" pad="72"/>
<connect gate="G$1" pin="VSS@86" pad="86"/>
<connect gate="G$1" pin="VSSQ@12" pad="12"/>
<connect gate="G$1" pin="VSSQ@32" pad="32"/>
<connect gate="G$1" pin="VSSQ@38" pad="38"/>
<connect gate="G$1" pin="VSSQ@46" pad="46"/>
<connect gate="G$1" pin="VSSQ@52" pad="52"/>
<connect gate="G$1" pin="VSSQ@6" pad="6"/>
<connect gate="G$1" pin="VSSQ@78" pad="78"/>
<connect gate="G$1" pin="VSSQ@84" pad="84"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IS45S32160F"/>
<attribute name="SUPPLIER" value="ISSI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429BIT6" prefix="U">
<description>STM32F429 Cortex-M4 CPU
180 MHz, 256 KB RAM, 2 MB Flash</description>
<gates>
<gate name="IO" symbol="STM32F429_LQFP-208_IO"/>
<gate name="CFG" symbol="STM32F429_LQFP-208_CFG"/>
<gate name="PWR" symbol="STM32F429_LQFP-208_PWR"/>
<gate name="FMC" symbol="STM32F429_LQFP-208_FMC"/>
</gates>
<devices>
<device name="" package="LQFP-208">
<connects>
<connect gate="CFG" pin="BOOT0@197" pad="197"/>
<connect gate="CFG" pin="NRST" pad="34"/>
<connect gate="CFG" pin="OSC_IN/PH0" pad="32"/>
<connect gate="CFG" pin="OSC_OUT/PH1" pad="33"/>
<connect gate="CFG" pin="PA13/JTMS-SWDIO" pad="147"/>
<connect gate="CFG" pin="PA14/JTCK-SWCLK" pad="159"/>
<connect gate="CFG" pin="PA15/JTDI" pad="160"/>
<connect gate="CFG" pin="PB2/BOOT1" pad="63"/>
<connect gate="CFG" pin="PB3/JTDO/TRACESWO" pad="192"/>
<connect gate="CFG" pin="PB4/NJTRST" pad="193"/>
<connect gate="CFG" pin="PDR_ON@203" pad="203"/>
<connect gate="CFG" pin="VREF+@41" pad="41"/>
<connect gate="FMC" pin="FMC_A0/PF0" pad="16"/>
<connect gate="FMC" pin="FMC_A1/PF1" pad="17"/>
<connect gate="FMC" pin="FMC_A10/PG0" pad="77"/>
<connect gate="FMC" pin="FMC_A11/PG1" pad="78"/>
<connect gate="FMC" pin="FMC_A12/PG2" pad="129"/>
<connect gate="FMC" pin="FMC_A13/PG3" pad="130"/>
<connect gate="FMC" pin="FMC_A14/PG4" pad="131"/>
<connect gate="FMC" pin="FMC_A15/PG5" pad="132"/>
<connect gate="FMC" pin="FMC_A16/PD11" pad="111"/>
<connect gate="FMC" pin="FMC_A17/PD12" pad="112"/>
<connect gate="FMC" pin="FMC_A18/PD13" pad="113"/>
<connect gate="FMC" pin="FMC_A19/PE3" pad="2"/>
<connect gate="FMC" pin="FMC_A2/PF2" pad="18"/>
<connect gate="FMC" pin="FMC_A20/PE4" pad="3"/>
<connect gate="FMC" pin="FMC_A21/PE5" pad="4"/>
<connect gate="FMC" pin="FMC_A22/PE6" pad="5"/>
<connect gate="FMC" pin="FMC_A23/PE2" pad="1"/>
<connect gate="FMC" pin="FMC_A24/PG13" pad="182"/>
<connect gate="FMC" pin="FMC_A25/PG14" pad="183"/>
<connect gate="FMC" pin="FMC_A3/PF3" pad="22"/>
<connect gate="FMC" pin="FMC_A4/PF4" pad="23"/>
<connect gate="FMC" pin="FMC_A5/PF5" pad="24"/>
<connect gate="FMC" pin="FMC_A6/PF12" pad="71"/>
<connect gate="FMC" pin="FMC_A7/PF13" pad="74"/>
<connect gate="FMC" pin="FMC_A8/PF14" pad="75"/>
<connect gate="FMC" pin="FMC_A9/PF15" pad="76"/>
<connect gate="FMC" pin="FMC_CLK/PD3" pad="167"/>
<connect gate="FMC" pin="FMC_NBL0/PE0" pad="200"/>
<connect gate="FMC" pin="FMC_NBL1/PE1" pad="201"/>
<connect gate="FMC" pin="FMC_NBL2/PI4" pad="205"/>
<connect gate="FMC" pin="FMC_NBL3/PI5" pad="206"/>
<connect gate="FMC" pin="FMC_NE1/PD7" pad="173"/>
<connect gate="FMC" pin="FMC_NL/PB7" pad="196"/>
<connect gate="FMC" pin="FMC_NOE/PD4" pad="168"/>
<connect gate="FMC" pin="FMC_NWAIT/PD6" pad="172"/>
<connect gate="FMC" pin="FMC_NWE/PD5" pad="169"/>
<connect gate="FMC" pin="PB5/FMC_SDCKE1" pad="194"/>
<connect gate="FMC" pin="PB6/FMC_SDNE1" pad="195"/>
<connect gate="FMC" pin="PC0/FMC_SDNWE" pad="35"/>
<connect gate="FMC" pin="PC2/FMC_SDNE0" pad="37"/>
<connect gate="FMC" pin="PC3/FMC_SDCKE0" pad="38"/>
<connect gate="FMC" pin="PD0/FMC_D2" pad="164"/>
<connect gate="FMC" pin="PD1/FMC_D3" pad="165"/>
<connect gate="FMC" pin="PD10/FMC_D15" pad="110"/>
<connect gate="FMC" pin="PD14/FMC_D0" pad="116"/>
<connect gate="FMC" pin="PD15/FMC_D1" pad="117"/>
<connect gate="FMC" pin="PD8/FMC_D13" pad="108"/>
<connect gate="FMC" pin="PD9/FMC_D14" pad="109"/>
<connect gate="FMC" pin="PE10/FMC_D7" pad="84"/>
<connect gate="FMC" pin="PE11/FMC_D8" pad="85"/>
<connect gate="FMC" pin="PE12/FMC_D9" pad="86"/>
<connect gate="FMC" pin="PE13/FMC_D10" pad="87"/>
<connect gate="FMC" pin="PE14/FMC_D11" pad="88"/>
<connect gate="FMC" pin="PE15/FMC_D12" pad="89"/>
<connect gate="FMC" pin="PE7/FMC_D4" pad="79"/>
<connect gate="FMC" pin="PE8/FMC_D5" pad="80"/>
<connect gate="FMC" pin="PE9/FMC_D6" pad="81"/>
<connect gate="FMC" pin="PF11/FMC_SDNRAS" pad="70"/>
<connect gate="FMC" pin="PG15/FMC_SDNCAS" pad="191"/>
<connect gate="FMC" pin="PG8/FMC_SDCLK" pad="135"/>
<connect gate="FMC" pin="PH10/FMC_D18" pad="100"/>
<connect gate="FMC" pin="PH11/FMC_D19" pad="101"/>
<connect gate="FMC" pin="PH12/FMC_D20" pad="102"/>
<connect gate="FMC" pin="PH13/FMC_D21" pad="151"/>
<connect gate="FMC" pin="PH14/FMC_D22" pad="152"/>
<connect gate="FMC" pin="PH15/FMC_D23" pad="153"/>
<connect gate="FMC" pin="PH8/FMC_D16" pad="98"/>
<connect gate="FMC" pin="PH9/FMC_D17" pad="99"/>
<connect gate="FMC" pin="PI0/FMC_D24" pad="154"/>
<connect gate="FMC" pin="PI1/FMC_D25" pad="155"/>
<connect gate="FMC" pin="PI10/FMC_D31" pad="12"/>
<connect gate="FMC" pin="PI2/FMC_D26" pad="156"/>
<connect gate="FMC" pin="PI3/FMC_D27" pad="157"/>
<connect gate="FMC" pin="PI6/FMC_D28" pad="207"/>
<connect gate="FMC" pin="PI7/FMC_D29" pad="208"/>
<connect gate="FMC" pin="PI9/FMC_D30" pad="11"/>
<connect gate="IO" pin="FMC_CD/PF9" pad="30"/>
<connect gate="IO" pin="FMC_INT2/PG6" pad="133"/>
<connect gate="IO" pin="FMC_INT3/PG7" pad="134"/>
<connect gate="IO" pin="FMC_INTR/PF10" pad="31"/>
<connect gate="IO" pin="FMC_NCE4_1/FMC_NE3/PG10" pad="179"/>
<connect gate="IO" pin="FMC_NCE4_2/PG11" pad="180"/>
<connect gate="IO" pin="FMC_NE2/FMC_NCE3/PG9" pad="178"/>
<connect gate="IO" pin="FMC_NE4/PG12" pad="181"/>
<connect gate="IO" pin="FMC_NIORD/PF6" pad="27"/>
<connect gate="IO" pin="FMC_NIOWR/PF8" pad="29"/>
<connect gate="IO" pin="FMC_NREG/PF7" pad="28"/>
<connect gate="IO" pin="FMC_SDCKE0/PH2" pad="46"/>
<connect gate="IO" pin="FMC_SDCKE1/PH7" pad="97"/>
<connect gate="IO" pin="FMC_SDNE1/PH6" pad="96"/>
<connect gate="IO" pin="I2C2_SCL/PH4" pad="48"/>
<connect gate="IO" pin="I2C2_SDA/PH5" pad="49"/>
<connect gate="IO" pin="PA4" pad="53"/>
<connect gate="IO" pin="PA8" pad="142"/>
<connect gate="IO" pin="PB0" pad="61"/>
<connect gate="IO" pin="PB1" pad="62"/>
<connect gate="IO" pin="PB10" pad="90"/>
<connect gate="IO" pin="PB11" pad="91"/>
<connect gate="IO" pin="PB12" pad="104"/>
<connect gate="IO" pin="PB8/I2C1_SCL" pad="198"/>
<connect gate="IO" pin="PB9/I2C1_SDA" pad="199"/>
<connect gate="IO" pin="PC1" pad="36"/>
<connect gate="IO" pin="PC13" pad="8"/>
<connect gate="IO" pin="PC14" pad="9"/>
<connect gate="IO" pin="PC15" pad="10"/>
<connect gate="IO" pin="PC4" pad="57"/>
<connect gate="IO" pin="PC5" pad="58"/>
<connect gate="IO" pin="PC6" pad="138"/>
<connect gate="IO" pin="PC7" pad="139"/>
<connect gate="IO" pin="PH3" pad="47"/>
<connect gate="IO" pin="PI11" pad="13"/>
<connect gate="IO" pin="PI12" pad="19"/>
<connect gate="IO" pin="PI13" pad="20"/>
<connect gate="IO" pin="PI14" pad="21"/>
<connect gate="IO" pin="PI15" pad="64"/>
<connect gate="IO" pin="PI8" pad="7"/>
<connect gate="IO" pin="PJ0" pad="65"/>
<connect gate="IO" pin="PJ1" pad="66"/>
<connect gate="IO" pin="PJ10" pad="122"/>
<connect gate="IO" pin="PJ11" pad="123"/>
<connect gate="IO" pin="PJ12" pad="174"/>
<connect gate="IO" pin="PJ13" pad="175"/>
<connect gate="IO" pin="PJ14" pad="176"/>
<connect gate="IO" pin="PJ15" pad="177"/>
<connect gate="IO" pin="PJ2" pad="67"/>
<connect gate="IO" pin="PJ3" pad="68"/>
<connect gate="IO" pin="PJ4" pad="69"/>
<connect gate="IO" pin="PJ5" pad="95"/>
<connect gate="IO" pin="PJ6" pad="118"/>
<connect gate="IO" pin="PJ7" pad="119"/>
<connect gate="IO" pin="PJ8" pad="120"/>
<connect gate="IO" pin="PJ9" pad="121"/>
<connect gate="IO" pin="PK0" pad="126"/>
<connect gate="IO" pin="PK1" pad="127"/>
<connect gate="IO" pin="PK2" pad="128"/>
<connect gate="IO" pin="PK3" pad="186"/>
<connect gate="IO" pin="PK4" pad="187"/>
<connect gate="IO" pin="PK5" pad="188"/>
<connect gate="IO" pin="PK6" pad="189"/>
<connect gate="IO" pin="PK7" pad="190"/>
<connect gate="IO" pin="SDIO_CK/PC12" pad="163"/>
<connect gate="IO" pin="SDIO_CMD/PD2" pad="166"/>
<connect gate="IO" pin="SDIO_D0/PC8" pad="140"/>
<connect gate="IO" pin="SDIO_D1/PC9" pad="141"/>
<connect gate="IO" pin="SDIO_D2/PC10" pad="161"/>
<connect gate="IO" pin="SDIO_D3/PC11" pad="162"/>
<connect gate="IO" pin="SPI1_MISO/PA6" pad="55"/>
<connect gate="IO" pin="SPI1_MOSI/PA7" pad="56"/>
<connect gate="IO" pin="SPI1_SCK/PA5" pad="54"/>
<connect gate="IO" pin="SPI2_MISO/PB14" pad="106"/>
<connect gate="IO" pin="SPI2_MOSI/PB15" pad="107"/>
<connect gate="IO" pin="SPI2_SCK/PB13" pad="105"/>
<connect gate="IO" pin="USART1_CTS/PA11" pad="145"/>
<connect gate="IO" pin="USART1_RTS/PA12" pad="146"/>
<connect gate="IO" pin="USART1_RX/PA10" pad="144"/>
<connect gate="IO" pin="USART1_TX/PA9" pad="143"/>
<connect gate="IO" pin="USART2_CTS/WKUP/PA0" pad="43"/>
<connect gate="IO" pin="USART2_RTS/PA1" pad="44"/>
<connect gate="IO" pin="USART2_RX/PA3" pad="50"/>
<connect gate="IO" pin="USART2_TX/PA2" pad="45"/>
<connect gate="PWR" pin="VBAT@6" pad="6"/>
<connect gate="PWR" pin="VCAP1@92" pad="92"/>
<connect gate="PWR" pin="VCAP2@148" pad="148"/>
<connect gate="PWR" pin="VDD@103" pad="103"/>
<connect gate="PWR" pin="VDD@115" pad="115"/>
<connect gate="PWR" pin="VDD@124" pad="124"/>
<connect gate="PWR" pin="VDD@137" pad="137"/>
<connect gate="PWR" pin="VDD@15" pad="15"/>
<connect gate="PWR" pin="VDD@150" pad="150"/>
<connect gate="PWR" pin="VDD@158" pad="158"/>
<connect gate="PWR" pin="VDD@171" pad="171"/>
<connect gate="PWR" pin="VDD@185" pad="185"/>
<connect gate="PWR" pin="VDD@204" pad="204"/>
<connect gate="PWR" pin="VDD@26" pad="26"/>
<connect gate="PWR" pin="VDD@39" pad="39"/>
<connect gate="PWR" pin="VDD@52" pad="52"/>
<connect gate="PWR" pin="VDD@59" pad="59"/>
<connect gate="PWR" pin="VDD@73" pad="73"/>
<connect gate="PWR" pin="VDD@83" pad="83"/>
<connect gate="PWR" pin="VDD@94" pad="94"/>
<connect gate="PWR" pin="VDDA@42" pad="42"/>
<connect gate="PWR" pin="VSS@114" pad="114"/>
<connect gate="PWR" pin="VSS@125" pad="125"/>
<connect gate="PWR" pin="VSS@136" pad="136"/>
<connect gate="PWR" pin="VSS@14" pad="14"/>
<connect gate="PWR" pin="VSS@149" pad="149"/>
<connect gate="PWR" pin="VSS@170" pad="170"/>
<connect gate="PWR" pin="VSS@184" pad="184"/>
<connect gate="PWR" pin="VSS@202" pad="202"/>
<connect gate="PWR" pin="VSS@25" pad="25"/>
<connect gate="PWR" pin="VSS@51" pad="51"/>
<connect gate="PWR" pin="VSS@60" pad="60"/>
<connect gate="PWR" pin="VSS@72" pad="72"/>
<connect gate="PWR" pin="VSS@82" pad="82"/>
<connect gate="PWR" pin="VSS@93" pad="93"/>
<connect gate="PWR" pin="VSSA@40" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_FARNELL" value="2469581"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232H">
<description>INTERFACE, USB - UART/FIFO</description>
<gates>
<gate name="G$1" symbol="FT232H"/>
</gates>
<devices>
<device name="" package="FT2323HL_LQFP48">
<connects>
<connect gate="G$1" pin="!RESET" pad="34"/>
<connect gate="G$1" pin="ACBUS0" pad="21"/>
<connect gate="G$1" pin="ACBUS1" pad="25"/>
<connect gate="G$1" pin="ACBUS2" pad="26"/>
<connect gate="G$1" pin="ACBUS3" pad="27"/>
<connect gate="G$1" pin="ACBUS4" pad="28"/>
<connect gate="G$1" pin="ACBUS5" pad="29"/>
<connect gate="G$1" pin="ACBUS6" pad="30"/>
<connect gate="G$1" pin="ACBUS7" pad="31"/>
<connect gate="G$1" pin="ACBUS8" pad="32"/>
<connect gate="G$1" pin="ACBUS9" pad="33"/>
<connect gate="G$1" pin="ADBUS0" pad="13"/>
<connect gate="G$1" pin="ADBUS1" pad="14"/>
<connect gate="G$1" pin="ADBUS2" pad="15"/>
<connect gate="G$1" pin="ADBUS3" pad="16"/>
<connect gate="G$1" pin="ADBUS4" pad="17"/>
<connect gate="G$1" pin="ADBUS5" pad="18"/>
<connect gate="G$1" pin="ADBUS6" pad="19"/>
<connect gate="G$1" pin="ADBUS7" pad="20"/>
<connect gate="G$1" pin="AGND@4" pad="4"/>
<connect gate="G$1" pin="AGND@41" pad="41"/>
<connect gate="G$1" pin="AGND@9" pad="9"/>
<connect gate="G$1" pin="DM" pad="6"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="EECLK" pad="44"/>
<connect gate="G$1" pin="EECS" pad="45"/>
<connect gate="G$1" pin="EEDATA" pad="43"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@36" pad="36"/>
<connect gate="G$1" pin="GND@47" pad="47"/>
<connect gate="G$1" pin="GND@48" pad="48"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="TEST" pad="42"/>
<connect gate="G$1" pin="VCCA" pad="37"/>
<connect gate="G$1" pin="VCCD" pad="39"/>
<connect gate="G$1" pin="VCCIO@12" pad="12"/>
<connect gate="G$1" pin="VCCIO@24" pad="24"/>
<connect gate="G$1" pin="VCCIO@46" pad="46"/>
<connect gate="G$1" pin="VCCORE" pad="38"/>
<connect gate="G$1" pin="VPHY" pad="3"/>
<connect gate="G$1" pin="VPLL" pad="8"/>
<connect gate="G$1" pin="VREGIN" pad="40"/>
<connect gate="G$1" pin="XCSI" pad="1"/>
<connect gate="G$1" pin="XCSO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_FARNELL" value="1870924"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232H_SERIAL" prefix="U">
<description>INTERFACE, USB - UART/FIFO</description>
<gates>
<gate name="G$1" symbol="FT232H_ASYNC_SERIAL"/>
</gates>
<devices>
<device name="" package="FT2323HL_LQFP48">
<connects>
<connect gate="G$1" pin="!RESET" pad="34"/>
<connect gate="G$1" pin="ACBUS1" pad="25"/>
<connect gate="G$1" pin="ACBUS2" pad="26"/>
<connect gate="G$1" pin="ACBUS5" pad="29"/>
<connect gate="G$1" pin="ACBUS6" pad="30"/>
<connect gate="G$1" pin="ACBUS8" pad="32"/>
<connect gate="G$1" pin="ACBUS9" pad="33"/>
<connect gate="G$1" pin="AGND@4" pad="4"/>
<connect gate="G$1" pin="AGND@41" pad="41"/>
<connect gate="G$1" pin="AGND@9" pad="9"/>
<connect gate="G$1" pin="CTS#" pad="16"/>
<connect gate="G$1" pin="DCD#" pad="19"/>
<connect gate="G$1" pin="DM" pad="6"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="DSR#" pad="18"/>
<connect gate="G$1" pin="DTR#" pad="17"/>
<connect gate="G$1" pin="EECLK" pad="44"/>
<connect gate="G$1" pin="EECS" pad="45"/>
<connect gate="G$1" pin="EEDATA" pad="43"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@36" pad="36"/>
<connect gate="G$1" pin="GND@47" pad="47"/>
<connect gate="G$1" pin="GND@48" pad="48"/>
<connect gate="G$1" pin="PWRSAV#" pad="31"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RI#" pad="20"/>
<connect gate="G$1" pin="RTS#" pad="15"/>
<connect gate="G$1" pin="RXD" pad="14"/>
<connect gate="G$1" pin="RXLED#" pad="27"/>
<connect gate="G$1" pin="TEST" pad="42"/>
<connect gate="G$1" pin="TXD" pad="13"/>
<connect gate="G$1" pin="TXDEN" pad="21"/>
<connect gate="G$1" pin="TXLED#" pad="28"/>
<connect gate="G$1" pin="VCCA" pad="37"/>
<connect gate="G$1" pin="VCCD" pad="39"/>
<connect gate="G$1" pin="VCCIO@12" pad="12"/>
<connect gate="G$1" pin="VCCIO@24" pad="24"/>
<connect gate="G$1" pin="VCCIO@46" pad="46"/>
<connect gate="G$1" pin="VCCORE" pad="38"/>
<connect gate="G$1" pin="VPHY" pad="3"/>
<connect gate="G$1" pin="VPLL" pad="8"/>
<connect gate="G$1" pin="VREGIN" pad="40"/>
<connect gate="G$1" pin="XCSI" pad="1"/>
<connect gate="G$1" pin="XCSO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_FARNELL" value="1870924"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
