<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<packages>
<package name="NDW">
</package>
<package name="NDY">
<description>NDY(11)</description>
</package>
<package name="QFN68_8X11X1.85">
<description>Altera EN5364QI 68-pin QFP</description>
</package>
<package name="QFN38_4X7X1.85">
</package>
<package name="TSOT-8-23">
</package>
</packages>
<symbols>
<symbol name="LMZ22005">
<pin name="VIN" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
<symbol name="LMZ22008">
<pin name="SYNC" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="SH"/>
<pin name="VOUT" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
</symbol>
<symbol name="EN5364QI">
<pin name="PVIN" direction="pwr"/>
<pin name="AVIN" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
<pin name="VFB"/>
<pin name="S_IN" direction="in"/>
<pin name="S_OUT" direction="out"/>
<pin name="EN_PB" direction="in"/>
<pin name="POK" direction="out"/>
<pin name="EAOUT" direction="out"/>
<pin name="OCP_ADJ" direction="in"/>
<pin name="MAR1" direction="in"/>
<pin name="MAR2" direction="in"/>
<pin name="VSENSE"/>
<pin name="S_DELAY" direction="in"/>
<pin name="M/S" direction="in"/>
</symbol>
<symbol name="EN6337QI">
<pin name="PVIN" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="AVIN" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
<pin name="VFB" direction="in"/>
<pin name="LLM/SYNC" direction="in"/>
<pin name="SS"/>
<pin name="POK" direction="out"/>
<pin name="RLLM" direction="in"/>
</symbol>
<symbol name="LT3060">
<pin name="REF/BYP" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="pwr"/>
<pin name="IN" direction="pwr"/>
<pin name="!SHDN" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LMZ22005">
<gates>
<gate name="G$1" symbol="LMZ22005"/>
</gates>
<devices>
<device name="" package="NDW">
<connects>
<connect gate="G$1" pin="AGND" pad="P$4"/>
<connect gate="G$1" pin="EN" pad="P$3"/>
<connect gate="G$1" pin="FB" pad="P$5"/>
<connect gate="G$1" pin="PGND" pad="P$8"/>
<connect gate="G$1" pin="SS/TRK" pad="P$6"/>
<connect gate="G$1" pin="SYNC" pad="P$2"/>
<connect gate="G$1" pin="VIN" pad="P$1"/>
<connect gate="G$1" pin="VOUT" pad="P$7"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_FARNELL" value="1890060"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMZ22008">
<gates>
<gate name="G$1" symbol="LMZ22008"/>
</gates>
<devices>
<device name="" package="NDY">
<connects>
<connect gate="G$1" pin="AGND" pad="P$5 P$6"/>
<connect gate="G$1" pin="EN" pad="P$4"/>
<connect gate="G$1" pin="FB" pad="P$7"/>
<connect gate="G$1" pin="PGND" pad="P$8"/>
<connect gate="G$1" pin="SH" pad="P$10"/>
<connect gate="G$1" pin="SS/TRK" pad="P$9"/>
<connect gate="G$1" pin="SYNC" pad="P$3"/>
<connect gate="G$1" pin="VIN" pad="P$1 P$2"/>
<connect gate="G$1" pin="VOUT" pad="P$11 P$12"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_FARNELL" value="2492265"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMZ13608">
<description>LMZ13608 8-A SIMPLE SWITCHER
Power Module With 36-V Maximum Input Voltage

http://www.ti.com/lit/ds/symlink/lmz13608.pdf</description>
<gates>
<gate name="G$1" symbol="LMZ22008"/>
</gates>
<devices>
<device name="" package="NDY">
<connects>
<connect gate="G$1" pin="AGND" pad="P$5 P$6"/>
<connect gate="G$1" pin="EN" pad="P$4"/>
<connect gate="G$1" pin="FB" pad="P$7"/>
<connect gate="G$1" pin="PGND" pad="P$8"/>
<connect gate="G$1" pin="SH" pad="P$10"/>
<connect gate="G$1" pin="SS/TRK" pad="P$9"/>
<connect gate="G$1" pin="SYNC" pad="P$3"/>
<connect gate="G$1" pin="VIN" pad="P$1 P$2"/>
<connect gate="G$1" pin="VOUT" pad="P$11 P$12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMZ13608TZ/NOPB"/>
<attribute name="OC_FARNELL" value="2492265"/>
<attribute name="PACKAGE" value="NDY (11)"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EN5364QI">
<description>6A PowerSoC
Voltage Mode Synchronous Buck PWM DC-DC Converter
With Integrated Inductor</description>
<gates>
<gate name="G$1" symbol="EN5364QI"/>
</gates>
<devices>
<device name="" package="QFN68_8X11X1.85">
<connects>
<connect gate="G$1" pin="AGND" pad="P$55"/>
<connect gate="G$1" pin="AVIN" pad="P$53"/>
<connect gate="G$1" pin="EAOUT" pad="P$57"/>
<connect gate="G$1" pin="ENABLE" pad="P$52"/>
<connect gate="G$1" pin="EN_PB" pad="P$51"/>
<connect gate="G$1" pin="M/S" pad="P$50"/>
<connect gate="G$1" pin="MAR1" pad="P$61"/>
<connect gate="G$1" pin="MAR2" pad="P$62"/>
<connect gate="G$1" pin="OCP_ADJ" pad="P$58"/>
<connect gate="G$1" pin="PGND" pad="P$1 P$2 P$3 P$4 P$27 P$28 P$29 P$30 P$31 P$32 P$33 P$64 P$65 P$66 P$67 P$68 P$69 P$70 P$71"/>
<connect gate="G$1" pin="POK" pad="P$54"/>
<connect gate="G$1" pin="PVIN" pad="P$34 P$35 P$36 P$37 P$38 P$39 P$40 P$41 P$42 P$43"/>
<connect gate="G$1" pin="SS" pad="P$59"/>
<connect gate="G$1" pin="S_DELAY" pad="P$60"/>
<connect gate="G$1" pin="S_IN" pad="P$49"/>
<connect gate="G$1" pin="S_OUT" pad="P$48"/>
<connect gate="G$1" pin="VFB" pad="P$56"/>
<connect gate="G$1" pin="VOUT" pad="P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12 P$13"/>
<connect gate="G$1" pin="VSENSE" pad="P$63"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EN5364QI"/>
<attribute name="OC_FARNELL" value="2081142"/>
<attribute name="PACKAGE" value="QFN"/>
<attribute name="SUPPLIER" value="ENPIRION"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EN6337QI">
<description>3A PowerSoC
Voltage Mode Synchronous PWM Buck with Integrated Inductor</description>
<gates>
<gate name="G$1" symbol="EN6337QI"/>
</gates>
<devices>
<device name="" package="QFN38_4X7X1.85">
<connects>
<connect gate="G$1" pin="AGND" pad="P$32"/>
<connect gate="G$1" pin="AVIN" pad="P$33"/>
<connect gate="G$1" pin="ENABLE" pad="P$27"/>
<connect gate="G$1" pin="LLM/SYNC" pad="P$26"/>
<connect gate="G$1" pin="PGND" pad="P$13 P$14 P$15 P$16 P$17 P$18 P$39 P$40"/>
<connect gate="G$1" pin="POK" pad="P$28"/>
<connect gate="G$1" pin="PVIN" pad="P$19 P$20 P$21"/>
<connect gate="G$1" pin="RLLM" pad="P$29"/>
<connect gate="G$1" pin="SS" pad="P$30"/>
<connect gate="G$1" pin="VFB" pad="P$31"/>
<connect gate="G$1" pin="VOUT" pad="P$5 P$6 P$7 P$8 P$9 P$10 P$11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EN6337QI"/>
<attribute name="PACKAGE" value="QFN"/>
<attribute name="SUPPLIER" value="ENPIRION"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EN6347QI">
<description>3A PowerSoC
Voltage Mode Synchronous PWM Buck with Integrated Inductor</description>
<gates>
<gate name="G$1" symbol="EN6337QI"/>
</gates>
<devices>
<device name="" package="QFN38_4X7X1.85">
<connects>
<connect gate="G$1" pin="AGND" pad="P$32"/>
<connect gate="G$1" pin="AVIN" pad="P$33"/>
<connect gate="G$1" pin="ENABLE" pad="P$27"/>
<connect gate="G$1" pin="LLM/SYNC" pad="P$26"/>
<connect gate="G$1" pin="PGND" pad="P$13 P$14 P$15 P$16 P$17 P$18 P$39 P$40"/>
<connect gate="G$1" pin="POK" pad="P$28"/>
<connect gate="G$1" pin="PVIN" pad="P$19 P$20 P$21"/>
<connect gate="G$1" pin="RLLM" pad="P$29"/>
<connect gate="G$1" pin="SS" pad="P$30"/>
<connect gate="G$1" pin="VFB" pad="P$31"/>
<connect gate="G$1" pin="VOUT" pad="P$5 P$6 P$7 P$8 P$9 P$10 P$11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EN6347QI"/>
<attribute name="OC_FARNELL" value="2081146"/>
<attribute name="PACKAGE" value="QFN"/>
<attribute name="SUPPLIER" value="ENPIRION"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3060?-*">
<description>Micropower, Low Noise, 100mA LDO, Linear Regulator</description>
<gates>
<gate name="G$1" symbol="LT3060"/>
</gates>
<devices>
<device name="" package="TSOT-8-23">
<connects>
<connect gate="G$1" pin="!SHDN" pad="7"/>
<connect gate="G$1" pin="ADJ" pad="2"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN" pad="5 6"/>
<connect gate="G$1" pin="OUT" pad="3 4"/>
<connect gate="G$1" pin="REF/BYP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LT3060ITS8-15#TRMPBF"/>
<attribute name="OC_FARNELL" value="2471073"/>
<attribute name="SUPPLIER" value="Linear Technology"/>
</technology>
</technologies>
</device>
<device name="ITS8" package="TSOT-8-23">
<connects>
<connect gate="G$1" pin="!SHDN" pad="7"/>
<connect gate="G$1" pin="ADJ" pad="2"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN" pad="5 6"/>
<connect gate="G$1" pin="OUT" pad="3 4"/>
<connect gate="G$1" pin="REF/BYP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="SUPPLIER" value="Linear Technology"/>
</technology>
<technology name="15">
<attribute name="MPN" value="LT3060ITS8-15#TRMPBF"/>
<attribute name="OC_FARNELL" value="2471073"/>
<attribute name="SUPPLIER" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
